WINDSHIELD GLASS REPLACEMENT FOR ALLANTE 1987. Cadillac Allante 1987

For 1990-2009 cars

# WINDSHIELD GLASS REPLACEMENT FOR ALLANTE 1987

#### MODELS AFFECTED: 1987 ALLANTE

A new windshield glass assembly, P/N 1644586, is available through GMSPO for the 1987 Allante . This assembly consists of the windshield glass, P/N 1635170, mirror plate, P/N 20626174, and a windshield upper reveat molding, P/N 1635180, which is bonded to the upper edge of the windshield glass.

When servicing the windshield glass, the windshield glass outer seal, P/N 1635173, must also be replaced.

For warranty purposes, use Labor Operation C0034 at 3.5 hours.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.