TRI-BAND ANTENNA SERVICE PARTS (PARTS ARE NOW AVAILABLE). Cadillac Allante 1987

For 1990-2009 cars

# TRI-BAND ANTENNA SERVICE PARTS (PARTS ARE NOW AVAILABLE)

#### SUBJECT: TRI-BAND (AM/FM/CELLULAR MOBILE TELEPHONE) ANTENNA SERVICE PARTS AVAILABILITY

Component parts are now available for repairing GM tri-band (AM/FM/cellular telephone) telescoping antennas. These antennas previously required replacement as a unit when the antenna had failed at the upper or lower load coil due to impact. Refer to Figure 1.

Applicable models with factory phone provisions are:

1987-1990 Cadillac Allantes 1988-1989 Cadillac Eldorados and Sevilles 1988-1989 Buick Rivieras

Upper Load Coil P/N: 22094783 Lower Load Coil P/N: 22094784

Installation instructions are included with these parts.

Parts are currently available from GMSPO.

| | WARRANTY INFORMATION | | VEHICLE SERIES | Operation | | | | | | Operation Description | Number | C | D | E | J | K | V ----------------------------|------------|----|----|-----|----|-----|---- Power, Loading Coil, Antenna| R0435 | | | | | | Components - Replace | | | | | | | Upper: | | | | .3 | | .3 | .3 Lower: | | | | .5 | | .5 | .5 Both: | | | | .7 | | .7 | .7 | | | | | | |

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.