FUEL FILLER DOOR DOESN'T OPEN PROPERLY. Cadillac Allante 1987

For 1990-2009 cars

# FUEL FILLER DOOR DOESN'T OPEN PROPERLY

FUEL FILLER DOOR DOESN'T OPEN PROPERLY

#### VEHICLES AFFECTED: 1987 ALLANTE ------------------ Some Allantes may experience a condition of the fuel filler door not springing open when the release button is pressed. This condition may be caused by a missing "n-shaped" assist spring contained in the latch assembly. To repair this condition, install a new assist spring, P/N 20355094, as shown in Figure 1.

Use the most applicable labour operation from the Canadian Labour Time Guide and claim 0.2 hours.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.