For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Fuse Block | Mounted to the I/P, lower LH side of the steering column | -- | --
Garage Door Opener | Located within the inside rear view mirror | -- | --
Inside Rear View Mirror | Attached to the upper center of the windshield | Power Roof Systems Component Views in Roof | Stationary Windows Connector End Views in Stationary Windows
C200A | I/P wiring harness to body wiring harness, at lower LH A-pillar | Power and Grounding Component Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G103 | Body and I/P wiring harness, located at the LH front of the engine compartment, underneath the battery tray | Wiper/Washer Component Views in Wiper/Washer System | --
P103 | Lower LH A-pillar, forward of G200 | Power and Grounding Component Views in Wiring Systems | --
S200 | I/P wiring harness, approximately 15 cm (6 in) from cruise release switch and stoplamp switch branch break off, towards G201 branch break off | -- | --
S308 | Body wiring harness, base of RH A-pillar, just under conduit | -- | --