For 1990-2009 cars

#### Line Pressure (4L30-E)

Transmission Mode | Selector Lever Position | Main Pressure (Pressure Gauge) | Pressure Control Solenoid Current (Amp)
--- | --- | --- | ---
Mode vs Pressure at Idle Speed
Economy/Sport | D, 3, 2, 1 | 450-750 kPa | 570-770 mA
Winter | D | 450-750 kPa | 570-770 mA
Economy/Sport | R | 300-400 kPa | 1008 mA
Mode vs Pressure at Stall Speed
Economy/Sport | D, 3, 2, 1 | 1150-1300 kPa | 115-170 mA
Winter | D | 1150-1300 kPa | 115-170 mA
Economy/Sport | R | 1170-1350 kPa | 290-320 mA