For 1990-2009 cars

Figure 1: |

#### Front Center Console

(1) | Heater and A/C Control
(2) | Electronic Traction Control Switch
(3) | Rear Compartment Lid Release Switch
(4) | Passenger Seat Heater Switch
(5) | Radio
(6) | Automatic Transmission Winter Mode Switch
(7) | LH Front Side Door Window Switch
(8) | Driver Seat Heater Switch
(9) | Fuel Tank Filler Door Lock Release Switch
(10) | Hazard Warning Switch

Figure 2: |

#### Rear Center Console

(1) | LH Front Side Door Window Switch Connector
(2) | RH Front Side Door Window Switch Connector
(3) | Park Brake Indicator Switch
(4) | Inflatable Restraint Sensing and Diagnostic and Seat Belt Pretensioner Module
(5) | Automatic Transmission Control Indicator
(6) | Body Wiring Harness

Figure 3: |

#### Engine Control Module (ECM)

(1) | ECM Connector C1 (Part of the Motronic Harness)
(2) | Engine Control Module
(3) | ECM Connector C2 (Part of the I/P Harness)
(4) | ECM Ground

Figure 4: |

#### Power Steering Control Module

(1) | Multifunction Relay K134
(2) | Passenger Seat Heater Relay K56
(3) | Driver Seat Heater Relay K55
(4) | Power Steering Control Module

Figure 5: |

#### Top View of Rear Engine

(1) | Coolant Bridge
(2) | Coolant Temperature Sender
(3) | Engine Coolant Temperature (ECT) Sensor

Figure 6: |

#### Washer Solvent Level Switch and Low Coolant Level Sensor

(1) | Energy Absorber
(2) | Windshield Washer Solvent Reservoir
(3) | Windshield Washer Solvent Level Switch
(4) | Low Coolant Level Sensor
(5) | Radiator Surge Tank

Figure 7: |

#### Brake Pad Wear Sensor

(1) | Speed Sensor Cable
(2) | Brake Pad Wear Sensor Cable
(3) | Brake Pad Wear Sensor