For 1990-2009 cars

### Removal Procedure

1. Remove the hinge cover from the rear seatback center armrest.

Use a small screwdriver in order to pry off the hinge cover.

2. Remove the rear seatback center armrest from the retainer.

### Installation Procedure

1. Install the rear back center armrest to the retainer.
2. Install the hinge cover to the rear seatback center armrest by pushing firmly on the cover.