For 1990-2009 cars

Causes | Action
--- | ---
The Selector Lever is in Position 2. | Adjust the Selector Lever Position Switch/Shift Linkage.
The Selector Lever Position Switch/Shift Linkage is incorrectly adjusted. | Refer to DTC P0758 2-3 Shift Solenoid Circuit Electrical .
The Solenoid Valve for the 2-3 Shift or the On-Off Valve in the Valve Body Assembly is defective. |

1. Find the defective part.
2. Replace the defective part.