For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
2. Remove the rear seatback outer cushion. Refer to Seat Back Cushion Replacement - Rear Outer .
3. Remove the retaining rings from the outer cushion cover of the rear seatback.
4. Remove the outer cushion cover of the rear seatback.

### Installation Procedure

1. Install the outer cushion cover of the rear seatback.
2. Install the retaining rings to the outer cushion cover of the rear seatback.
3. Install the rear seatback outer cushion. Refer to Seat Back Cushion Replacement - Rear Outer .
4. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .