For 1990-2009 cars

#### A/T Range Switch

Connector Part Information |

• | ZPF 8-3

• | 8-Way F

Pin | Wire Color | CircuitNo. | Function
--- | --- | --- | ---
A | BLK/BLU | FP733 | Transmission Position Signal
B | BLK/GRN | FU726 | Transmission Position Signal
C | BLK/YEL | FB708 | Transmission Position Signal
D | BRN | X756 | B+ from Fuse #3
E | BLK/RED | FA501 | Starter Solenoid Signal
F | WHT/BLK | MF757 | Rear View Mirror/Backup Lamp Supply Voltage
G | GRY | R733 | Transmission Position Signal
H | BLK/RED | FA500 | B+ in the ON Position

#### Ambient Light Sunload Sensor

Connector Part Information |

• | F4-21

• | 4-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN | X812 | 5 V Reference
2 | BLK/WHT | FM60 | Sun Sensor Input Signal
3 | BLK | F830 | TS Day/Night Signal
4 | BLU | P111 | Sensor Ground

#### Aux Brake Lamp

Connector Part Information |

• | ZPM 2-50

• | 2-Way M (WHT)

Pin | Wire Color | CircuitNo. | Function
--- | --- | --- | ---
A | BLK | F3 | Ground to G400
B | BLK/YEL | FB15 | Backup Lamp Supply Voltage

#### Backup/Tail Lamp - Left

Connector Part Information |

• | PF 2-1

• | 3-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
H | BLK | F2 | Ground to G400
J | GRY/GRN | RU2 | Lamp ON Signal
K | WHT/BLK | MF1 | Lamp ON Feed

#### Backup/Tail Lamp - Right

Connector Part Information |

• | PF 2-1

• | 2-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
H | BLK | F1 | Ground to G400
J | GRY/GRN | RU3 | Lamp ON Signal
K | WHT/BLK | MF10 | Lamp ON Feed
WHT/BLK | MF1 | Lamp ON Feed

#### Cornering Lamp - Left

Connector Part Information |

• | ZFW 2-9

• | 2-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY/BLK | RF1 | Cornering Lamp Supply Voltage
2 | BLK | F2 | Ground to G103

#### Cornering Lamp - Right

Connector Part Information |

• | ZFW 2-9

• | 2-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY/RED | RA1 | Lamp ON Signal
2 | BLK | F5 | Ground to G103

#### Daytime Running Lamp (DRL) Relay K133

Connector Part Information |

• | ZFW 5-20

• | 5-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WHT | M70 | Relay Control
2 | WHT | M65 | DRL High Beam Series Circuit
3 | RED | A832 | B+ from Fuse #21
4 | BLK | F803 | Ground to G103
5 | BLK/WHT | FM19 | LH Headlamp Control Ground

#### Dome and Reading Lamps

Connector Part Information |

• | BLK F 4-21

• | 4-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN/BLU | XP806 | Interior Lamps Relay Output Ground
2 | BLK | F901 | Ground to G103
3 | RED/BLU | AP882 | Courtesy Lamps Supply Voltage
4 | RED/BLU | AP808 | Courtesy Lamps Supply Voltage

#### Door Jamb Switch - Driver

Connector Part Information |

• | F 2-42

• | 2-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY/WHT | RM2 | Door Open Signal
2 | GRY | R2 | Door Jamb Signal

#### Door Jamb Switch - Front Passenger

Connector Part Information |

• | F 2-42

• | 2-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | GRY | R6 | Door Open Signal

#### Door Jamb Switch - LR

Connector Part Information |

• | F 2-42

• | 2-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY | R2 | Door Open Signal
2 | GRY | R1 | Door Open Signal

#### Door Jamb Switch - RR

Connector Part Information |

• | F 2-42

• | 2-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY | R2 | Door Open Signal
2 | GRY | R1 | Door Jamb Signal

#### Fog Lamp - Left

Connector Part Information |

• | ZFW 2-10

• | 2-Way F (BLU)

Pin | Wire Color | CircuitNo. | Function
--- | --- | --- | ---
1 | BRN | X2 | Lamp ON Signal
2 | BLK | F3 | Ground to G103

#### Fog Lamp - Right

Connector Part Information |

• | ZFW 2-10

• | 2-Way F (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRN | X3 | Lamp ON Signal
2 | BLK | F4 | Ground to G103

#### Hazard Warning Switch

Connector Part Information |

• | ZF 9-4

• | 9-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/WHT | FM22 | Turn Signal Flasher Signal Circuit
2 | BLK | F27 | Ground to G103
3 | BLU | P3 | Ignition Positive Voltage
4 | BLK/WHT | FM3 | Hazard Switch LH Signal
5 | -- | -- | Not Used
6 | RED | A9 | B+ from Fuse #12
7 | BLK/GRN | FU3 | Hazard Switch RH Signal
8 | GRY/YEL | RB77 | Interior Lamps Dimming Control
GRY/YEL | RB70 | Interior Lamps Dimming Control
9 | BRN | X10 | B+ from Fuse #3

#### Headlamp - Left

Connector Part Information |

• | ZPF 5-1

• | 5-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | BLK/WHT | FM13 | High Beam Signal
C | YEL | B1 | Low Beam Signal (w/o T97)
D | BLK | F840 | Ground to G103
E | WHT | M2 | High Beam Signal

#### Headlamp - Right

Connector Part Information |

• | ZPF 5-1

• | 5-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | BLK | F11 | Ground to G103
C | YEL | B3 | Low Beam Voltage (w/o T97)
D | -- | -- | Not Used
E | WHT | M1 | RH High Beam Supply Voltage

#### Headlamp Relay - LH K73 - High Beam

Connector Part Information |

• | ZFW 5-20

• | 5-Way F

Pin | Wire Color | CircuitNo. | Function
--- | --- | --- | ---
1 | BRN/PPL | XY802 | Relay Control
2 | -- | -- | Not Used
3 | RED | A825 | B+ from Fuse #21
4 | WHT | M8 | LH High Beam Supply Voltage
5 | RED | A10 | B+ from Fuse #21

#### Headlamp Relay - RH K132 - High Beam

Connector Part Information |

• | ZF 9-14

• | 9-Way F (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | RED | A850 | B+ from Fuse #32
3 | -- | -- | Not Used
4 | RED | A827 | B+ from Fuse #32
5 | BLK/RED | FA888 | Switched Battery Voltage for Fog Lamps
6 | WHT | M62 | Relay Control
7 | -- | -- | Not Used
8 | WHT | M64 | RH High Beam Supply Voltage
WHT | M65 | RH High Beam Supply Voltage
9 | -- | -- | Not Used

#### Headlamp Switch

Connector Part Information |

• | ZF 18-7

• | 18-Way F (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY/GRN | RU70 | B+ from Fuse #26
2 | GRY/YEL | RB1 | Interior Lamps Dimming Control
3 | BRN | X22 | B+ from Fuse #15
4 | BRN/RED | XA811 | Low Beam Relay Control Signal
5 | BRN/WHT | XM815 | Park Lamp Relay Control Signal
6 | YEL | B60 | Low Beam ON/OFF Signal
7 | RED/WHT | AM813 | Park Lamp ON/OFF Signal
8 | BRN/PPL | XY112 | Interior Lamps Switch Signal
9 | RED/YEL | AB810 | TS ON/OFF Signal
10 | BLK/BLU | FP28 | Fog Lamp Switch Signal
11 | BLK/BRN | FX810 | TS Delay Signal
12 | BLK/PPL | FY810 | TS Return Signal
13 | BLK | F18 | Ground to G103
14 | YEL | B55 | B+ form Fuse #22
15 | -- | -- | Not Used
16 | BRN/BLK | XF830 | TS Indicator
17 | RED | A5 | B+ from Fuse #8
18 | GRY/WHT | RM901 | Chime Control Signal

#### I/P Compartment Lamp

Connector Part Information |

• | F 2-14

• | 2-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED/BLU | AP802 | Courtesy Lamps Supply Voltage
B | BLK | F72 | IP Compartment Lamp Switch Signal

#### I/P Compartment Lamp Switch

Connector Part Information |

• | F 2-14

• | 2-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | F71 | Ground to G103
B | BLK | F72 | IP Compartment Lamp Switch Signal

#### Low Beam Relay K131

Connector Part Information |

• | ZFW 5-20

• | 5-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN/RED | XA810 | Relay Control
BRN/RED | XA811 | Relay Control
2 | -- | -- | Not Used
3 | RED/WHT | AM811 | Exterior Lamp Power
4 | YEL | B50 | Low Beam Supply Voltage
5 | RED | A814 | B+ from Fuse V3

#### Multifunction Relay K134

Connector Part Information |

• | F 14-3

• | 14-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/RED | FA888 | Switched Battery Positive Voltage
2 | RED/BLU | AP805 | Courtesy Lamps Supply Voltage
3 | GRY/BLK | RF75 | Park Lamp Supply voltage
4 | BRN | X6 | Fog Lamp Supply Voltage
5 | RED | A831 | B+ from Fuse #29
6 | BLK | F805 | Ground to G103
7 | BRN/PPL | XY800 | Delayed Interior Lamp Relay Control
8 | BLK/BLU | FP28 | Fog Lamp Switch Signal
9 | BRN/PPL | XY801 | Interior Lamp Relay Control
10 | BRN | X820 | Ignition Voltage from Fuse #15
11 | BRN/BLU | XP810 | Battery Guard Signal
12 | RED | A821 | B+ from Fuse #8
13 | BRN/BLU | XP803 | Rear Compartment Open Signal
14 | RED | A600 | Low Power Drive Signal

#### Park Lamp Relay K130

Connector Part Information |

• | ZFW 5-20

• | 5-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN/WHT | XM810 | Relay Control
BRN/WHT | XM815 | Relay Control
2 | -- | -- | Not Used
3 | RED/WHT | AM810 | Exterior Lamp Power
RED/WHT | AM811 | Exterior Lamp Power
4 | GRY/GRN | RU812 | Park Lamp Supply Voltage
5 | RED | A813 | B+ from Fuse V3

#### Park/Turn Signal Lamp - LF

Connector Part Information |

• | ZFW 3-21

• | 3-Way F (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | F12 | Ground to G103
B | GRY/BLK | RF3 | Park Lamp Signal
C | BLK/WHT | FM2 | Park Lamp Signal

#### Park/Turn Signal Lamp - RF

Connector Part Information |

• | ZFW 3-21

• | 3-Way F (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | F16 | Ground to G103
B | GRY/RED | RA3 | Park Lamp Signal
C | BLK/GRN | FU2 | Park Lamp Signal

#### Side Marker Lamp - Left

Connector Part Information |

• | ZFW 2-9

• | 2-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/WHT | FM1 | Ground
2 | GRY/GRN | RU2 | Lamp ON Signal

#### Side Marker Lamp - Right

Connector Part Information |

• | ZFW 2-9

• | 2-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/GRN | FU1 | Ground
2 | GRY/GRN | RU3 | Lamp ON Signal

#### Stop Lamp Switch

Connector Part Information |

• | ZF 4-6

• | 4-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RED | A401 | B+ from Fuse #12
2 | BLK/YEL | FB101 | Brake Lamp Supply Voltage
3 | BRN | X120 | B+ from Fuse #2
4 | BLK/BRN | FX102 | RTSI Signal

#### Sunshade Illuminated Mirror Lamp - Left

Connector Part Information |

• | ZPF 2-50

• | 2-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | F3 | Ground to G103
B | RED/BLU | AP3 | Courtesy Lamps Supply Voltage

#### Sunshade Illuminated Mirror Lamp - Right

Connector Part Information |

• | ZPF 2-50

• | 2-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | F1 | Ground to G103
B | RED/BLU | AP1 | B+ from Multifunction Relay

#### Tail/Stop/Turn Lamp - Left

Connector Part Information |

• | ZPF 6-55

• | 6-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK | F125 | Ground to G400
2 | BLK/YEL | FB6 | Stop Lamp Signal
3 | BRN/WHT | XM101 | Hazard Flasher Signal
4 | -- | -- | Not Used
5 | GRY/BLK | RF4 | Lamp ON Signal
6 | BLU/WHT | FM20 | Left Turn Signal

#### Tail/Stop/Turn Lamp - Right

Connector Part Information |

• | ZPF 6-55

• | 6-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK | F25 | Ground to G400
2 | BLK/YEL | FB2 | Stop Lamp Signal
3 | BRN/WHT | XM102 | Hazard Flasher Signal
4 | -- | -- | Not Used
5 | GRY/RED | RA4 | Lamp ON Signal
6 | BLK/GRN | FU20 | Right Turn Signal

#### Turn Signal/Hazard Flasher Module K10

Connector Part Information |

• | ZF 9-14

• | 9-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BRN/WHT | XM200 | Hazard Flasher Signal
3 | -- | -- | Not Used
4 | BLK | F12 | Ground to G103
5 | -- | -- | Not Used
6 | BLU | P3 | Ignition Voltage
7 | -- | -- | Not Used
8 | BLK/WHT | FM22 | Hazard Flasher Signal
BLK/WHT | FM91 | Hazard Flasher Signal
9 | -- | -- | Not Used

#### Turn Signal Switch

Connector Part Information |

• | ZF 10-3

• | 10-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YEL | B905 | B+ from Fuse #31
2 | WHT | M3 | High Beam ON/OFF Signal
3 | YEL | B800 | B+ from Fuse #31
YEL | B905 | B+ from Fuse #31
4 | BLK/WHT | FM91 | Turn Signal Flasher Signal
5 | RED | A8 | B+ from Fuse #8
6 | -- | -- | Not Used
7 | GRY/RED | RA999 | RH Cornering Lamp Supply Voltage
8 | BLK/GRN | FU1 | RH Turn Lamp Supply Voltage
9 | BLK/WHT | FM1 | LH Turn Lamp Supply Voltage
10 | GRY/BLK | RH999 | LH Cornering Lamp Supply Voltage