For 1990-2009 cars

### Tubing and Fittings

The tubing connects to the air dryer. The tubing routes to a tee on the rear of the vehicle along the length of the right-hand frame by snap-in provisions on the brake/fuel/vapor clips. The tubing connects the rear shock absorbers from the tee. The tubing includes spring clip connections with molded sealing shoulders in the retainer.

Clean the connector and clean the surrounding area before disconnecting any tubing. Squeeze the spring clip in order to release the connector. Using petroleum jelly, lightly lubricate the tubing and push the tubing and the connector fully into the fitting.