For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
A/C Compressor Refrigerant Pressure Switch | LH front of the engine compartment, mounted in the A/C compressor/condenser hose, below the A/C load switch | Cooling System Component Views | Cooling System Connector End Views
Auxiliary Engine Coolant Fan #1 | Front of the LH side of the radiator | Cooling System Component Views | Cooling System Connector End Views
Auxiliary Engine Coolant Fan #2 | Front of the RH side of the radiator | Cooling System Component Views | Cooling System Connector End Views
Auxiliary Water Pump Relay K22 | LH front of the engine compartment, in the ECM housing | -- | Cooling System Connector End Views
Battery | LH front of the engine compartment | -- | --
Coolant Fan Test Connector | LH front of the engine compartment, in the ECM housing | -- | Cooling System Connector End Views
ECM Housing | LH front of the engine compartment | Cooling System Component Views | --
Electric Cooling Fan | Front center of the engine compartment, behind the radiator | Cooling System Component Views | Cooling System Connector End Views
Engine Coolant Fan Resistor | LH side of the engine compartment, mounted beneath the battery | Cooling System Component Views | --
Fan Control Relay K26 | LH front of the engine compartment, in the ECM housing | -- | Cooling System Connector End Views
Fan Control Relay K28 | LH front of the engine compartment, in the ECM housing | -- | Cooling System Connector End Views
Fan Control Relay K52 | LH front of the engine compartment, in the ECM housing | -- | Cooling System Connector End Views
Fan Control Relay K67 | LH front of the engine compartment, in the ECM housing | -- | Cooling System Connector End Views
Fan Control Relay K87 | LH front of the engine compartment, in the ECM housing | -- | Cooling System Connector End Views
Fuse 40 | LH front of the engine compartment, in the ECM housing |  | --
Fuse 42 | LH front of the engine compartment, in the ECM housing | -- | --
Fuse 50 | LH front of the engine compartment, in the ECM housing | -- | --
Fuse 52 | LH front of the engine compartment, in the ECM housing | -- | --
Fuse Block | Mounted to the I/P, lower LH side of the steering column | -- | --
Heater Water Auxiliary Pump | LH front of the engine compartment | Cooling System Component Views | Cooling System Connector End Views
Primary Coolant Fan Temperature Switch | In the upper LH side of the radiator | Cooling System Component Views | Cooling System Connector End Views
Secondary Coolant Fan Temperature Switch | In the lower LH side of the radiator | Cooling System Component Views | --
Water Auxiliary Pump | LH front of the engine compartment, to the right of the battery | -- | Cooling System Connector End Views
C200B | I/P wiring harness to body wiring harness, at lower LH A-pillar | Power and Grounding Component Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G103 | Body and I/P wiring harness, located at the LH front of the engine compartment, underneath the battery tray | Wiper/Washer Component Views in Wipers/Washer Systems | --
S108 | A/C control wiring harness, approximately 12 cm (5 in) from the C111 branch break off | -- | --
S109 | A/C control wiring harness, located between branch break off for the cooling fan resistor and branch break off for connectors C101 and C111 | -- | --
S110 | A/C control wiring harness, approximately 12 cm (5 in) from the C111 branch break off | -- | --
S111 | A/C control wiring harness, approximately 12 cm (5 in) from the C111 branch break off | -- | --
S112 | A/C control wiring harness, inside the ECM housing, near P104 | -- | --
S113 | A/C control wiring harness, inside the ECM housing, near P104 | -- | --
S114 | A/C control wiring harness, inside the ECM housing, near P104 | -- | --
S115 | A/C control wiring harness, inside the ECM housing, near P104 | -- | --
S116 | A/C control wiring harness, inside the ECM housing, near P104 | -- | --
S117 | A/C control wiring harness, inside the ECM housing, near P104 | -- | --
S118 | A/C control wiring harness, inside the ECM housing, near P104 | -- | --
S125 | A/C control wiring harness, approximately 12 cm (5 in) from the C111 branch break off | -- | --
S137 | A/C control wiring harness, approximately 12 cm (5 in) from the C111 branch break off | -- | --