For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Fascia Extension Screws | 3 N·m | 27 lb in
Front Bumper Energy Absorber Nuts | 27 N·m | 20 lb ft
Front Bumper Guard Bolts | 12 N·m | 108 lb ft
Front Bumper Impact Bar Nuts | 150 N·m | 111 lb ft
Front Fascia Center Lower Screw | 3 N·m | 27 lb in
Front Fascia Lower Screw | 3 N·m | 27 lb in
Front Fascia Retainer Screws | 10 N·m | 89 lb in
Front Fascia-to-Fender Screws | 3 N·m | 27 lb in
Rear Bumper Energy Absorber Nuts | 27 N·m | 20 lb ft
Rear Bumper Impact Bar Nuts | 20 N·m | 15 lb ft
Rear Fascia Retainer Screws | 10 N·m | 89 lb in
Rear Fascia-to-Body Screws | 3 N·m | 27 lb in
Windshield Washer Fluid Reservoir Nuts | 3 N·m | 27 lb in