For 1990-2009 cars

#### Door Lock Relay K135

Connector Part Information |

• | F 14-3

• | 14 WAY F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/RED BRN/PPL | FA811 XY804 | Fuel Door Release Input Signal from the Body Control Module and Trunk Release Button
2 | BLK/RED | FA809 | Unlock Door Output Signal to Driver's Door Actuator
3 | -- | -- | Not Used
4 | BRN/PPL | XY803 | Driver's Door Unlock Signal from the Body Control Module
5 | RED | A888 | Battery Power Input
6 | BLK/RED | FA805 | Fuel Door Unlock Signal to the Fuel Lid Actuator
7 | BRN/PPL | XY807 | Doors Unlock Input Signal from the Body Control Module
8 | RED | A911 | Ignition Power Input
9 | BLK/RED BRN/PPL | FA812 XY805 | Trunk Lid Lock Release Input Signal from the Body Control Module and Fuel Lid Unlock Button
10 | BLK/RED | FA801 | Unlock Door Output Signal to Passenger and Rear Door Actuators
11 | BRN/PPL | XY806 | Doors Lock Input Signal from Body Control Module
12 | BLK/YEL | FB801 | Doors Lock Output Signal to All Doors and Fuel Lid
13 | BLK/RED | FA807 | Trunk Lid Lock Output Signal to the Trunk Lid Actuator
14 | BLK | F911 | Ground

#### Driver Seat Adjuster Memory Module (Connector C2)

Connector Part Information |

• | ZF 26-2

• | 26 WAY F

Pin | Wire Color | Circuit No. | Function | Component Connector Cavity | DTC(s) Affected | Possible Symptoms From a Faulty Circuit
--- | --- | --- | --- | --- | --- | ---
1-3 |  |  | Not Used |  |  |
4 | BLK/BRN | FX75 | Memory Pot Signal |  | 18, 19 and 20 | All Memory Mirrors Become Disabled
5 | BRN | X75 | Memory Pot Signal |  | 18, 19 and 20 | All Memory Mirrors Become Disabled
6 | GRY/GRN | RU60 | Memory Pot Signal |  | 20 | RH Outside Memory Mirror Becomes Disabled
7 | GRY | R70 | Memory Pot Signal |  | 20 | RH Outside Memory Mirror Becomes Disabled
8 | GRY/BLK | RF60 | Memory Pot Signal |  | 19 | Inside Memory Mirror Becomes Disabled
9 | GRY/YEL | RB60 | Memory Pot Signal |  | 19 | Inside Memory Mirror Becomes Disabled
10 | GRY/GRN | RU50 | Memory Pot Signal |  | 18 | LH Outside Memory Mirror Becomes Disabled
11 | GRY | R60 | Memory Pot Signal |  | 18 | LH Outside Memory Mirror Becomes Disabled
12 |  |  | Not Used |  |  |
13 | BLK/RED | FA75 | Memory Mirror Common |  |  |
14-20 |  |  | Not Used |  |  |
21 | GRN | U80 | LH Mirror Control Signal |  |  |
22 | YEL | B12 | LH Mirror Control Signal |  |  |
23 | BLU/WHT | PM60 | Inside Mirror Control Signal |  |  |
24 | BLU/RED | PA60 | Inside Mirror Control Signal |  |  |
25 | BLU | P70 | RH Mirror Control Signal |  |  |
26 | GRY | R65 | RH Mirror Control Signal |  |  |

#### LH Front Side Door Jamb Switch

Connector Part Information |

• | F 2-42

• | 2 WAY F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY/WHT | RM2 | Door Open Signal
2 | GRY | R2 | Door Open Signal

#### LH Front Side Door Lock Actuator

Connector Part Information |

• | ZFW 6-6

• | 6 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BLK/RED | FA809 | Door Unlock Signal
3-5 | -- | -- | Not Used
6 | BLK/YEL | FB9 | Door Lock Signal

#### LH Front Side Door Lock Switch

Connector Part Information |

• | F 4-21

• | 4 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/BRN | FX805 | Door Lock Signal
2 | BLK/PPL | FY805 | Door Unlock Signal
3 | RED/BLU | AP807 | Illumination Signal
4 | BLK | F12 | Ground to G200

#### LH Front Side Door Window Regulator Motor

Connector Part Information |

• | ZFW 6-6

• | 6 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RED | A2 | B+ from Fuse #1
2 | GRY/GRN | RU6 | Window Up Signal
3 | BLU/RED | PA2 | Window Down Signal
4 | BLK | F11 | Ground to G200
5 | YEL | B11 | B+ Input, Power Window Regulator Enable Signal
6 | -- | -- | Not Used

#### LH Front Side Door Window Switch

Connector Part Information |

• | ZF 9-21

• | 9 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLU/RED | PA2 | LH Front Door Window Motor Control
2 | GRY/GRN | RU5 | LH Front Door Window Motor Control
3 | BLU/RED | PA3 | LH Rear Door Window Motor Control
4 | GRY/GRN | RU15 | LH Rear Door Window Motor Control
5 | WHT | M5 | Rear Window Switch Voltage
6 | BRN | X2 | B+ from Fuse #15
7 | RED | A3 | B+ from Fuse #1
8 | -- | -- | Not Used
9 | GRY | R10 | All Door Jamb Signal

#### LH Outside Rear View Mirror (With Memory)

Connector Part Information |

• | ZF 9-21

• | 9 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YEL | B20 | Motor Control
2 | GRN | U200 | Motor Control
3 | BLK/RED | FA81 | Motor Common
4 | BRN | X60 | Memory Pot Signal
5 | BLK/BRN | FX60 | Memory Pot Signal
6 | GRY | R60 | Memory Pot Signal
7 | GRY/GRN | RU60 | Memory Pot Signal
8 | BLK/WHT | FM15 | Defogger On Signal
9 | BLK | F50 | Ground to G200

#### LH Outside Rear View Mirror (Without Memory)

Connector Part Information |

• | ZF 9-21

• | 9 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YEL | B2 | Motor control
2 | GRN | U1 | Motor Control
3 | BLK/RED | FA4 | Motor Common
4-7 | -- | -- | Not Used
8 | BLK/WHT | FM2 | Defogger On Signal
9 | BLK | F2 | Ground to G200

#### LH Rear Side Door Lock Actuator

Connector Part Information |

• | ZFW 6-6

• | 6 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BLK/RED | FA804 | Door Lock Signal
3-5 | -- | -- | Not Used
6 | BLK/YEL | FB805 | Door Unlock Signal

#### LH Rear Side Door Window Regulator Motor

Connector Part Information |

• | ZFW 6-6

• | 6 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RED | A1 | B+ from Fuse #7
2 | GRY/GRN | RU2 | Window Up Signal
3 | BLU/RED | PA2 | Window Down Signal
4 | BLK | F1 | Ground to G200
5 | YEL | B1 | B+ Input, Power Window Regulator Enable Signal
6 | -- | -- | Not Used

#### LH Rear Side Door Window Switch

Connector Part Information |

• | ZM 9-5

• | 9 WAY M

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY/GRN | RU1 | Window Up Signal
2 | -- | -- | Not Used
3 | BLK | F2 | Ground to G200
4-6 | -- | -- | Not Used
7 | WHT | M1 | Power from Main Switch
8 | -- | -- | Not Used
9 | BLU/RED | PA1 | Window Down Signal

#### Outside Remote Control Rear View Mirror Switch

Connector Part Information |

• | F 8-17

• | 8 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN | X10 | Fused Battery Voltage
2 | BLK | F5 | Ground to G200
3 | GRY | R11 | RH Mirror Control
4 | GRN | U1 U10 | LH Mirror Control
5 | BLK/RED | FA2 | Mirror Common
6 | -- | -- | Not Used
7 | YEL | B2 B10 | LH Mirror Control
8 | BLU | P3 | RH Mirror Control

#### RH Front Side Door lock Actuator

Connector Part Information |

• | ZFW 6-6

• | 6 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BLK/RED | FA809 | Door Lock Signal
3-5 | -- | -- | Not Used
6 | BLK/YEL | FB9 | Door Lock Signal

#### RH Front Side Door Lock Switch

Connector Part Information |

• | F 4-21

• | 4 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/BRN | FX805 | Door Lock Signal
2 | BLK/PPL | FY805 | Door Unlock Signal
3 | RED/BLU | AP807 | Illumination Signal
4 | BLK | F12 | Ground to G200

#### RH Front Side Door Window Regulator Motor

Connector Part Information |

• | ZFW 3-6

• | 3 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RED | A2 | B+ from Fuse #1
2 | GRY/GRN | RU6 | Window Up Signal
3 | BLU/RED | PA2 | Window Down Signal
4 | BLK | F11 | Ground to G200
5 | YEL | B2 | B+ Input, Power Window Regulator Enable Signal
6 | -- | -- | Not Used

#### RH Front Side Door Window Switch

Connector Part Information |

• | ZPF 6-55

• | 6 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLU/RED | PA1 | RH Front Side Door Window Control
2 | GRY/GRN | RU6 | RH Front Side Door Window Control
3 | BLU/RED | PA4 | RH Rear Side Door Window Control
4 | GRY/GRN | RU16 | RH Rear Side Door Window Control
5 | BLK | F22 | Ground to G200
6 | YEL | B9 | B+ Voltage Feed

#### RH Outside Rear View Mirror (With Memory)

Connector Part Information |

• | ZF 9-21

• | 9 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY | R5 | Motor Control
2 | BLU | P10 | Motor Control
3 | BLK/RED | FA65 | Motor Common
4 | BRN | X65 | Memory Pot Signal
5 | BLK/BRN | FX65 | Memory Pot Signal
6 | GRY | R70 | Memory Pot Signal
7 | GRY/GRN | RU60 | Memory Pot Signal
8 | BLK/WHT | FM20 | Defogger On Signal
9 | BLK | F55 | Ground to G200

#### RH Outside Rear View Mirror (Without Memory)

Connector Part Information |

• | ZF 9-21

• | 9 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY | R4 | Motor Control
2 | BLU | P2 | Motor Control
3 | BLK/RED | FA4 | Motor Common
4-7 | -- | -- | Not Used
8 | BLK/WHT | FM2 | Defogger On Signal
9 | BLK | F2 | Ground to G200

#### RH Rear Side Door Lock Actuator

Connector Part Information |

• | ZFW 6-6

• | 6 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BLK/RED | FA804 | Door Lock Signal
3-5 | -- | -- | Not Used
6 | BLK/YEL | FB805 | Door Unlock Signal

#### RH Rear Side Door Window Regulator Motor

Connector Part Information |

• | ZFW 6-6

• | 6 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RED | A1 | B+ from Fuse #7
2 | GRY/GRN | RU2 | Window Up Signal
3 | BLU/RED | PA2 | Window Down Signal
4 | BLK | F1 | Ground to G200
5 | YEL | B1 | B+ Input, Power Window Regulator Enable Signal
6 | -- | -- | Not Used

#### RH Rear Side Door Window Switch

Connector Part Information |

• | ZM 9-5

• | 9 WAY M

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY/GRN | RU1 | Window Up Signal
2 | -- | -- | Not Used
3 | BLK | F2 | Ground to G200
4-6 | -- | -- | Not Used
7 | WHT | M1 | Power from Main Switch
8 | -- | -- | Not Used
9 | BLU/RED | PA1 | Window Down Signal

#### Stop Lamp Switch

Connector Part Information |

• | ZF 4-6

• | 4 WAY F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RED | A401 | B+ from Fuse #12
2 | BLK/YEL | FB101 | Brake Lamp ON Signal
3 | BRN | X120 | Fused Battery Voltage
4 | BLK/BRN | FX102 | BTSI Signal