For 1990-2009 cars

1. Remove the converter housing to the oil pump bolts (5).
2. Separate the oil pump (10) from the converter housing (6).
3. Remove the converter housing to oil pump outer seal (8).
4. Remove the oil pump body wear plate (9).
5. Remove the converter housing assembly seal ring screw (2).
6. Remove the converter housing assembly seal (3).
7. Inspect the converter housing (6) for wear and damage.