For 1990-2009 cars

Not all of the tools listed are required for this specific application. If a special tool is required, the J number will be called out in the diagnostic procedure. A tool's abilities and limitations must be known before the tool is used. This knowledge should include the scan tool operation, the proper use of test lights, the jumper wires, and the DVM.

For information regarding the use of a particular scan tool, refer to the documentation provided with the tool by the manufacturer.

Illustration | Tool Number/ Description
--- | ---
| J 23738-A/BT-8512-A Vacuum Pump
| J 26792/BT-7220-1 Spark Tester
| J 28742-A Weather Pack Terminal Remover
| J 33095/BT-8234-A Control Module Connector Terminal Remover
| J 34142-B Unpowered Test Light
| J 34730-1A Fuel Pressure Gauge
| J 34730-2C Injector Test Light
| J 35314-A Exhaust Pressure Tester
| J 35616-A/BT - 8637 Connector Test Adaptor Kit
| J 35689-A Metri-Pack Terminal Remover
| J 37287-100 Fuel Line Shut-Off Quick Connect Adaptors
| J 37287 Inlet and Return Fuel Line Shut-Off Adaptors
| J 38522 Variable Signal Generator
| J 39021 Fuel Injector Coil/Balance Test
| J 39021-210 Injector Switch Box
| J39021-360 Injector Harness Adaptor
| J 39194 Oxygen Sensor Wrench
| J 39200 High Impedance Multimeter (Digital Voltmeter - DVM
| J 41416 Ultrasonic Leak Detector
| J 41750 EVAP Pressure/Purge Cart
| J 42219 Fuel Sender Locknut Wrench
| J 42242 Fuel Pressure Gauge Adaptor
| J 42250 Terminal Repair Kit
| J 42374 Fuel Line Quick Connect Seperators
| J 42960-1 Fuel Tank Drain Hose
| 70000081 Tech II Scan Tool