For 1990-2009 cars

#### Line Pressure (4L30-E)

Transmission Mode | Selector Lever Position | Main Pressure (Pressure Gauge) | Pressure Control Solenoid Current (Amp)
--- | --- | --- | ---
Mode vs Pressure at Idle Speed
Economy/Sport | D, 3, 2, 1 | 1000-1100 kPa | 165 mA
Winter | D | 300-350 kPa | 970 mA
Economy/Sport | R | 400-500 kPa | 970 mA
Mode vs Pressure at Stall Speed
Economy/Sport | D, 3, 2, 1 | 1000-1100 kPa | 165 mA
Winter | D | 1000-1100 kPa | 165 mA
Economy/Sport | R | 1450-1550 kPa | 165 mA