For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Brake Fluid Minimum Capacity Sensor | Part of the brake master cylinder reservoir cap | Wiper/Washer System Component Views in Wiper/Washer System | Brake Warning System Connector End Views in Hydraulic Brakes
Fuse Block | Mounted to the I/P, lower LH side of the steering column | -- | --
Instrument Cluster | LH side of the I/P, above the steering column | -- | Instrument Cluster Connector End Views in Instrument Panel, Gauges and Console
Park Brake Indicator Switch | Attached to the park brake lever, in the center console | Instrument Cluster Component Views in Instrument Panel, Gauges and Console | --
C200A | I/P wiring harness, approximately 15 cm (6 in) from cruise release switch and stoplamp switch branch break off, towards G201 branch break off | Power and Grounding Component Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G103 | Body and I/P wiring harness, located at the LH front of the engine compartment, near C102, C105, and C106 | Wiper/Washer System Component Views in Wiper/Washer System | --
P110 | Rear LH corner of the engine compartment | -- | --
S140 | I/P wiring harness, near the brake fluid minimum capacity sensor connector branch break off | -- | --
S200 | I/P wiring harness, approximately 15 cm (6 in) from cruise release switch and stoplamp switch branch break off, towards G201 branch break off | -- | --
S237 | I/P wiring harness, near the multifunction relay K134 connector branch break off | -- | --