For 1990-2009 cars

#### Automatic Transmission Range Switch

Connector Part Information |

• | ZPF 8-3

• | 8 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/BLU | FP733 | Transmission Position Signal
B | BLK/GRN | FU726 | Transmission Position Signal
C | BLK/YEL | FB708 | Transmission Position Signal
D | BRN | X756 | B+ from Fuse #3
E | BLK/RED | FA501 | Starter Solenoid Signal
F | BLK/WHT | MF757 | Rear View Mirror Signal
G | GRY | R733 | Transmission Position Signal
H | BLK/RED | FA500 | B+ in the ON Position

#### Heated Outside Rear View Mirror and Rear Window Defogger Relay K35

Connector Part Information |

• | ZF 6-14

• | 6 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN | X84 | B+ from Fuse #14
2 | RED | A18 | B+ from Fuse #34
3 | -- | -- | Not Used
4 | BLK/WHT | FM14 | Defogger Switch Input
5 | BLK/WHT | FM10 | Heated Mirrors ON Signal
6 | BLK | F84 | Ground to G103
7 | -- | -- | Not Used
8 | BRN | X15 | Rear Defogger ON Signal

#### Heater and A/C Control Connector C1

Connector Part Information |

• | F 22-1

• | 22 WAY F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BLK | F830 | Twilight Sensor Signal
3 | BLK/WHT | FM60 | Sun Sensor Signal
4 | BRN/BLU | XP33 | T/S Day/Night Signal
5 | BLU | P11, P111 | Ground
6 | BLK/WHT | FM11 | B+ from Fuse #11
7 | BRN | X812 | +5 V reference
8 | GRY/GRN | RU502 | B+ from Fuse #26
9 | YEL/BLU | BP900 | A/C Cutout Signal
10 | BLK/WHT | FM7 | A/C Request Signal
11 | BLK/BLU | FP812 | Blower Output Signal
12 | BLU/WHT | PM4 | Outside Temperature Signal
13 | BRN/WHT | XM112 | Blower Diagnostics Input
14 | BLK/WHT | FM14 | Rear Window Defogger Switch Signal
15 | GRY/YEL | RB400 | Interior Lamps Dimming Signal
16 | -- | -- | Not Used
17 | BRN/WHT | XM110 | Serial Data
18 | BLU/RED | PA400 | Vehicle Speed Signal
19 | BRN | X800 | Ignition Positive Voltage
20 | GRN | U10 | RPM Signal Input
21 | BLK | F800 | Ground to G103
22 | RED | A400 | B+ from Fuse #12

#### Inside Rear View Mirror (with memory)

Connector Part Information |

• | F 12-3

• | 12 WAY F (BLK)

Pin | Wire Color | Circuit No. | Function | Component Connector Cavity | DTC(s) Affected | Possible Symptoms From a Faulty Circuit
--- | --- | --- | --- | --- | --- | ---
1 | BLU/RED | PA60 | Mirror Motor Control | 24 | -- | --
2 | BLU/WHT | PM60 | Mirror Motor Control | 23 | -- | --
3 | BLK/RED | FA70 | Mirror Motor Control | 13 | -- | --
4 | BRN | X70 | Memory Potentiometer Signal | 5 | DTC 18, 19, 20 | Inside and Outside Mirrors Inoperative
5 | BLK/BRN | FX70 | Memory Potentiometer Signal | 4 | DTC 18, 19, 20 | Inside and Outside Mirrors Inoperative
6 | GRY/YEL | RB60 | Memory Potentiometer Signal | 9 | DTC 19 | Inside Mirror Inoperative
7 | GRY/BLK | RF60 | Memory potentiometer signal | 8 | DTC 19 | Inside Mirror Inoperative
8 | BLK | F915 | Ground to G103 | -- | -- | --
9 | BRN/BLU | XP900 | B+ from Park Lamp Relay | -- | -- | --
10 | WHT/BLK | MF900 | Transmission Position Signal | -- | -- | --
11 | BRN | X900 | B+ from Fuse #15 | -- | -- | --
12 |  |  | Not Used | -- | -- | --