For 1990-2009 cars

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
ABS Warning Lamp | -- | Commands the ABS indicator ON and OFF.
Left Front Solenoid | -- | Commands the solenoid ON and OFF.
Left Rear Solenoid | -- | Commands the solenoid ON and OFF.
Pump Motor | -- | Commands the pump motor ON and OFF.
LF Inlet Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
LF Outlet Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
LR Inlet Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
LR Outlet Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
LF Master Cylinder Isolation Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
LF Prime Solenoid | Solenoid Test | Commands the solenoid ON and OFF.
TCS On/Off test | -- | Commands the traction control system ON and OFF. Performs the same function as the traction control switch.