For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Automatic Transmission Shift Lock Control Switch | Attached to the automatic transmission control base, to the right of the shift lever | -- | --
Body Control Module (BCM) | Mounted on the lower RH A-pillar, behind the trim panel | Body Control System Component Views in Body Control System | Body Control System Connector End Views in Body Control System
Door Lock Relay K135 | Mounted on the lower RH A-pillar, behind the BCM | Body Control System Component Views in Body Control System | Body Control System Connector End Views in Body Control System
Front Side Door Lock Switch (RH) | Mounted inside of the RH front side door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Fuel Tank Filler Door Lock Actuator | Inside the RH side of the rear compartment, near the fuel door | -- | Body Rear End Connector End Views
Fuel Tank Filler Door Lock Release Switch | Center of the I/P, to the left of the heater and A/C control | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | Body Rear End Connector End Views
Rear Compartment Lid Lock Release Actuator | Attached to the rear compartment lid | -- | Body Rear End Connector End Views
Rear Compartment Lid Release Switch | Center of the I/P, to the right of the heater and A/C control | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | Body Rear End Connector End Views
Rear Sunshade Motor | Mounted on the rear deck under trim panel | -- | --
C200A | I/P wiring harness to body wiring harness, at lower LH A-pillar | Power and Grounding Component Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200B | I/P wiring harness to body wiring harness, at lower LH A-pillar | Power and Grounding Component Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C205 | I/P wiring harness to automatic transmission control switches, attached to the automatic transmission control base, to the right of the shift lever | -- | Inline Harness Connector End Views in Wiring Systems
C405 | Body wiring harness to rear compartment lid wiring harness, on the rear compartment lid, under the trim panel, next to the LH backup lamp | -- | Inline Harness Connector End Views in Wiring Systems
G103 | Body and I/P wiring harness, located at the LH front of the engine compartment, underneath the battery tray | Wiper/Washer Component Views in Wipers/Washer System | --
G400 | Body wiring harness, in the lower LH corner of the rear compartment, near the LH stop/taillamp | -- | --
P103 | Lower LH A-pillar, forward of G200 | Power and Grounding Component Views in Wiring Systems | --
P110 | Rear LH corner of the engine compartment | -- | --
P401 | Lower LH corner of the rear compartment | -- | --
P402 | Upper LH corner of the rear compartment, near the LH stop/taillamp | -- | --
S103 | Body wiring harness, approximately 27 cm (10 in) from P107 | -- | --
S140 | I/P wiring harness, near the brake fluid minimum capacity sensor connector branch break off | -- | --
S250 | I/P wiring harness, near the gauge cluster connector branch break off | -- | --
S251 | I/P wiring harness, near the G201 branch break off | -- | --
S252 | I/P wiring harness, near the G201 branch break off | -- | --
S304 | Body wiring harness, approximately 23 cm (8 in) from the RCDLR branch break off | -- | --
S307 | Body wiring harness, base of RH A-pillar, just under conduit | -- | --