For 1990-2009 cars

## Instrument Panel, Gages, and Console Connector End Views Gauge Cluster Connector

#### Gauge Cluster Connector

Connector Part Information | ZF 26 - 1
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BRN/YEL | XB3 | WSWA solvent level signal
2 | YEL/RED | BA2 | Brake pad wear signal
3 | BRN/BLU | XP2 | Low level coolant signal
4 | BRN/GRN | XU600 | Oil level signal
5 | RED | A900 | Switched ignition from terminal W
6 | BLK | F8 | Ground (G103)
7-8 | Not Used |  |
9 | BLU/RED | PA600 | Vehicle speed signal
10-12 | Not Used |  |
13 | GRN | U5 | Tachometer signal
14 | BRN/BLK | XF20 | Seat belt signal
15 | BLU/GRN | PU1 | Oil pressure switch signal
16 | GRY/WHT | RM900 | Headlamps ON Chime signal
17 | GRY/YEL | RB103 | Interior lamps dinning signal
18 | BLU/WHT | PM1 | Generator signal
19 | Not Used
20 | BRN | X70 | Switched ignition from terminal 15
21 | BRN/PPL | XY2 | ALC sensor signal
22 | RED | A16 | B+ from fuse # 12
23 | BRN/BLU | XP840 | Security lamp indicator
24 | BLK | F11 | Lamp ground
25 | Not Used
26 | BLU/YEL | PB90 | Oil pressure sensor signal

## Instrument Panel, Gages, and Console Connector End Views Instrument Cluster Connector

#### Instrument Cluster Connector

Connector Part Information | M 26 - 1
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BRN/YEL | XB4 | ABS indicator signal
2 | BRN/YEL | XB105 | Traction control indicator signal
3 | GRY | R133 | Transmission malfunction indicator signal
4 | BLK/YEL | FB800 | Automatic transmission indicator (sport mode)
5 | BLK/BLU | FP40 | Fog lamp indicator
6 | BLK/WHT | FM13 | LH turn indicator
7 | BLK | F2 | Ground (G103)
8 | GRY/YEL | RB104 | Interior lamps dimming signal
9 | WHT | M75 | High beam relay signal
10 | BRN/BLU | XP900 | Rear compartment release signal
11 | RED/BLU | XP808 | Rear compartment release signal
12 | BRN/YEL | XB910 | Headlamps ON required signal
13 | BRN/YEL | XB20 | Airbag indicator signal
14 | BRN/BLU | XP21, XP22 | MIL control signal
15 | BRN/RED, BRN/WHT | XA2, XM2 | Brake on indicator
16 | BLK/RED | FA825 | Brake to shift signal
17 | BRN/BLU | XP950 | Cruise control indicator signal
18 | BLK/GRN | FU7 | RH turn indicator
19 | BRN | X13 | Switch ignition from terminal 15a
20 | BLU/BLK | PF!, PF10 | Low fuel signal
21 | BLU | P900 | Coolant temperature signal
22 | GRN | U4 | Tachometer signal
23 | BLU/RED | PA6 | Vehicle speed signal
24 | BRN/WHT | XM500 | Serial data
25 | RED | A971 | B+ from fuse # 12
26 | BLK | F300 | Controller ground to G103