For 1990-2009 cars

#### Horn #1

Connector Part Information |

• | ZPF 2-4

• | 2 WAY F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN/WHT | XM65 | Horn Signal
2 | RED | A17 | B+ from Fuse #17

#### Horn #2

Connector Part Information |

• | ZPF 2-4

• | 2 WAY F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN/WHT | XM60 | Horn Signal
2 | RED | A18 | B+ from Fuse #17

#### Horn Relay K63

Connector Part Information |

• | ZF 9-14

• | 9 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | RED | A121 | B+ from Fuse #8
3 | -- | -- | Not Used
4 | BRN/WHT | XM30 | Horn ON Signal
5 | -- | -- | Not Used
6 | BRN/WHT | XM1 XM899 | Switch Signal
7 | -- | -- | Not Used
8 | BLK | F700 | Ground to G103
9 | -- | -- | Not Used

#### Inflatable Restraint Steering Wheel Module Coil

Connector Part Information |

• | ZF 8-5

• | 8 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK | F122 | Ground to G201
2 | BRN/WHT | XM1 | Horn Relay Control Signal
3 | RED/WHT | AM116 | LED Control Signal
4 | BLU/RED | PA101 | Steering Wheel Switch Signal
5-6 | -- | -- | Not Used
7 | YEL/WHT | BM 30 | Driver Front Airbag High Signal
8 | YEL | B30 | Driver Front Airbag Low Signal