For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
ABS Sensor Bolt | 7 N·m | 62 lb in
Differential Ring Gear Bolt | 115 N·m | 85 lb ft
Differential Support Bracket Lower Bolt | 90 N·m first pass, 38° second pass | 66 lb ft first pass, 38° second pass
Differential Support Bracket Upper Bolt | 100 N·m | 74 lb ft
Height Sensor Bolt | 14 N·m | 124 lb in
Rear Axle Housing Cover Bolt | 60 N·m | 44 lb ft
Rear Axle Housing Filler Plug | 22 N·m | 15 lb ft
Rear Differential Bushing Bolt | 100 N·m | 74 lb ft