For 1990-2009 cars

#### Door Lock Relay K135

Connector Part Information |

• | F 14-3

• | 14 WAY F

• | BLK

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/RED BRN/PPL | FA811 XY804 | Fuel Door Release Input Signal from the Body Control Module and Trunk Release Button
2 | BLK/RED | FA809 | Unlock Door Output Signal to Driver's Door Actuator
3 | -- | -- | Not Used
4 | BRN/PPL | XY803 | Driver's Door Unlock Signal from the Body Control Module
5 | RED | A888 | Battery Power Input
6 | BLK/RED | FA805 | Fuel Door Unlock Signal to the Fuel Lid Actuator
7 | BRN/PPL | XY807 | Doors Unlock Input Signal from the Body Control Module
8 | RED | A911 | Ignition Power Input
9 | BLK/RED BRN/PPL | FA812 XY805 | Trunk Lid Lock Release Input Signal from the Body Control Module and Fuel Lid Unlock Button
10 | BLK/RED | FA801 | Unlock Door Output Signal to Passenger and Rear Door Actuators
11 | BRN/PPL | XY806 | Doors Lock Input Signal from Body Control Module
12 | BLK/YEL | FB801 | Doors Lock Output Signal to All Doors and Fuel Lid
13 | BLK/RED | FA807 | Trunk Lid Lock Output Signal to the Trunk Lid Actuator
14 | BLK | F911 | Ground

#### Fuel Tank Filler Door Lock Actuator

Connector Part Information |

• | F 6-11

• | 6 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/YEL | FB807 | Ground
B | BLK/RED | FA805 | Release signal
C-F | -- | -- | Not Used

#### Fuel Tank Filler Door Lock Release Switch

Connector Part Information |

• | ZF 10-7

• | 10 WAY F

• | BLK

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not used
2 | YEL | B901 B902 | Ground
3 | BLK/RED | FA811 | Release signal, Fuel door
4 | GRY/YEL | RB31 | Dimmer signal
5 | BLK | F54 | Ground to G103
6 | BLK/RED | --FB700 | Heater ON Signal
7 | BRN | X39 | B+ From Fuse 14
8 | BLK/RED | FA90 | Relay ON Signal
9 | GRY/YEL | RB30 RB31 | Dimmer Signal
10 | BLK | F53 F54 | Ground to G103

#### Rear Compartment Lid Lock Release Actuator

Connector Part Information |

• | PF 2-41

• | 2 WAY F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/YEL | FB21 | Ground
2 | BLK/RED | FA11 | Release Signal

#### Rear Window Sunshade Module C1

Connector Part Information |

• | ZF 3-6

• | 3 WAY F

• | BLK

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN | F20 | Ground
2 | RED | A95 | Fused Battery Voltage
3 | BLU/RED | PA6 | Sunshade Signal

#### Rear Window Sunshade Module C2

Connector Part Information |

• | ZF 2-3

• | 2 WAY F

• | WHT

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRN | -- | Sunshade Motor Signal
2 | WHT | -- | Sunshade Motor Signal

#### Rear Compartment Lid Release Switch

Connector Part Information |

• | ZF 10-6

• | 10 WAY F

• | BLU

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not used
2 | YEL | B902 | Fuel door release signal
3 | BLK/RED | FA812 | Rear compartment release relay signal
4 | GRY/YEL | RB33 | Rear compartment release switch indicator
5 | BLK | F56 | Ground to G103
6 | BLK/YEL | FB700 | Dimmer control signal
7 | BRN | X42 | B+ from fuse #14
8 | BLK/YEL | FB70 | Heater relay ON signal
9 | GRY/YEL | RB33 RB32 | Rear compartment release switch indicator
10 | BLK | F55 F56 | Ground to G103