For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Accelerator Pedal Position (APP) Sensor | Top of the Accelerator pedal, on the mounting bracket | -- | Engine Controls Connector End Views in Engine Controls
Cruise Control Switch | LH side of the steering column | -- | Cruise Control Connector End Views in Cruise Control
Cruise Control Release Switch | Attached to the brake pedal bracket assembly | -- | Cruise Control Connector End Views in Cruise Control
Engine Control Module (ECM) | LH front of the engine compartment , in the ECM housing | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Engine Control Module (ECM) C1 | LH front of the engine compartment, in the ECM housing | Cruise Control Component Views in Cruise Control | Engine Controls Connector End Views in Engine Controls
Engine Control Module (ECM) C2 | LH front of the engine compartment, in the ECM housing | Cruise Control Component Viewsin Cruise Control | Engine Controls Connector End Views in Engine Controls
Fuse Block | Mounted to the I/P, lower LH side of the steering column | -- | --
Instrument Cluster | LH side of the I/P, above the steering column | -- | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges and Console
Stop Lamp Switch | Attached to the brake pedal bracket assembly | -- | Lighting Systems Connector End Views in Lighting Systems
Throttle Position (TP) Sensor | Attached to the throttle body | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
P104 | In the LH engine compartment, in the ECM housing | -- | --
S121 | ECM wiring harness, inside the ECM housing, approximately 4 cm (2 in) from P108 | -- | --
S200 | I/P wiring harness, approximately 15 cm (6 in) from cruise release switch and stoplamp switch branch break off, towards G201 branch break off | -- | --
S206 | I/P wiring harness, approximately 22 cm (9 in) from P110, towards connector C200 branch break off | -- | --
S208 | I/P wiring harness, in stop lamp switch branch break off | -- | --
S229 | I/P wiring harness mounted in harness channel behind LH side of heater and A/C control unit, approximately 25 cm (10 in) from cruise release switch and stoplamp switch branch break off | -- | --
S253 | I/P wiring harness, approximately 28 cm (11 in) from cruise release switch and stoplamp switch branch break off, towards G201 branch break off | -- | --