For 1990-2009 cars

Table 1: | Camshaft Position (CMP) Sensor
Table 2: | Crankshaft Position (CKP) Sensor
Table 3: | Engine Control Module (ECM)
Table 4: | Engine Controls Power Relay K43
Table 5: | Engine Coolant Temperature (ECT) Sensor
Table 6: | Engine Oil Level Sensor
Table 7: | Evaporative (EVAP) Purge Solenoid Valve
Table 8: | Evaporative (EVAP) Tank Solenoid Valve
Table 9: | Fuel Injector #1
Table 10: | Fuel Injector #2
Table 11: | Fuel Injector #3
Table 12: | Fuel Injector #4
Table 13: | Fuel Injector #5
Table 14: | Fuel Injector #6
Table 15: | Fuel Pump
Table 16: | Fuel Pump Relay K44
Table 17: | Fuel Tank Pressure Sensor
Table 18: | Heated Oxygen Sensor (Bank 1, Position 1)
Table 19: | Heated Oxygen Sensor (Bank 2, Position 1)
Table 20: | Heated Oxygen Sensor (Bank 2, Position 2)
Table 21: | Heated Oxygen Sensor (Bank 1, Position 2)
Table 22: | Idle Air Control (IAC) Valve
Table 23: | Ignition Coil
Table 24: | Intake Air Temperature (IAT) Sensor
Table 25: | Intake Plenum Switch-Over Solenoid Valve
Table 26: | Intake Resonance Switch-Over Valve Solenoid Valve
Table 27: | Knock Sensor (Bank 1)
Table 28: | Knock Sensor (Bank 2)
Table 29: | Mass Air Flow (MAF) Sensor
Table 30: | Secondary Air Injection Pump
Table 31: | Secondary Air Injection Pump Relay K12
Table 32: | Secondary Air Injection Pump Solenoid Valve
Table 33: | Throttle Position Sensor

#### Camshaft Position (CMP) Sensor

Connector Part Information | ZFW 3-23
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BLK | S11 | Shield wire
2 | GRY/BLK | RF381 | CMP sensor signal
3 | RED/GRY | RA543 | Positive battery voltage

#### Crankshaft Position (CKP) Sensor

Connector Part Information | ZFW 3-23
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | GRY/BLK | RF78 | CKP sensor signal
2 | GRY/RED | RA20 | Reference low signal
3 | BLK | S03 | Positive battery voltage

#### Engine Control Module (ECM)

Connector Part Information | ZFW 8-88
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BRN/WHT | XM1 | HO2S Heater Control
2 | BRN/BLU | XP2 | IAC Valve CLOSED Signal
3 | BRN/YEL | XB17 | Fuel Injector #1 Control
4 | BRN/BLU | XP35 | Fuel Injector #3 Control
5 | BLU/BLK | XF35 | Fuel Injector #5 Control
6 | BLK | F6 | Ground to G102
7 | BRN/GRN | XU7 | Intake Resonance Switch-over Solenoid Valve Control
8 | BRN/BLU | XP8 | MIL Control Signal
9-11 | -- | -- | NOT USED
12 | BLK/BLU | FP120 | A/C Request Signal
13-14 | -- | -- | NOT USED
15 | BLK/WHT | FM430 | A/C Request Input
16 | BLU/RED | PA16 | IAT Sensor Signal
17 | BLU/GRN | PU7 | MAF Sensor Signal`
18 | BRN/BLU | XP18 | HO2S Signal
19 | BRN/BLU | XP19 | HO2S Signal
20 | GRY/RED | RA20 | CKP Sensor Ground
21 | BRN/GRN | XU21 | Torque Control Input
22-25 | -- | -- | NOT USED
26 | RED/YEL | AB26 | Battery Positive Voltage
27 | BRN/GRY | XR46 | Fuel Injector Relay Control
28 | BLK | F28 | Ground to G102
29 | BRN/RED | XA29 | IAC Valve OPEN Signal
30 | BRN/WHT | XM30 | HO2S Heater Control
31 | BRN/GRN | XU16 | Fuel Injector #2 Control
32 | BRN/RED | XA34 | Fuel Injector #4 Control
33 | BRN/PPL | XY33 | Fuel Injector #6 Control
34 | BLK | F34 | Ground to G102
35 | BRN/GRN | XU35 | Intake Plenum Switch-over Solenoid Valve Control
36 | BRN/PPL | XY360 | A/C Compressor Relay Control
37 | PPL | Y370 | Secondary Air Injection Pump Control
38 | GRY/BLK | RF381 | CMP Sensor Signal
39 | BLU | P390 | MIL Input Signal
40 | BRN/WHT | XM40 | KS Bank 2 Signal
41-43 | -- | -- | NOT USED
44 | BRN/BLU | XP53 | TP Sensor Signal
45 | BRN/GRN | XY306 | MAF Sensor Ground
46 | BRN/GRN | XY46 | HO2S Ground
47 | -- | -- | NOT USED
48 | GRY | R48 | Desired Engine Torque Input
49 | GRY/BLK | RF1 | 1-4 Ignition Control
50 | BLK/YEL | FB20 | 2-5 Ignition Control
51 | BLK/RED | FA21 | 6-3 Ignition Control
52 | -- | -- | Not used
53 | BLU/BLK | PF53 | +5 V reference
54 | RED/BLU GRY/RED | AP54 RA543 | Positive Battery Voltage
55 | BLK | F55 | Ground to G101
56 | BRN | X56 | Ignition Positive Voltage
57-60 | -- | -- | NOT USED
61 | BRN/RED | XA61 | EVAP Purge Solenoid Valve Control
62 | PPL | Y67 | Secondary Air Injection Pump Valve Control
63 | BRN/BLU | XP3 | Fuel Pump Relay Control
64 | -- | -- | NOT USED
65 | BRN/BLK | XF65 | EVAP Tank Solenoid Valve Control
66-68 | -- | -- | NOT USED
69 | BLK/RED | FA69 | P/N Input
70 | BRN/WHT | XM70 | KS Bank 1 Signal
71 | BRN/GRN | XU400 | KS Gound
72 | BRN/YEL | XB72 | Fuel Pressure Sensor Signal
73 | BLU/BLK | PF73 | Fuel Level Output Signal
74 | BRN/BLU | XP74 | ECT Sensor Signal
75 | -- | -- | NOT USED
76 | BRN/BLU | XP76 | HO2S Signal
77 | BRN/BLU | XP77 | HO2S Signal
78 | GRY/WHT | RF78 | CKP Sensor Signal
79 | BLU/RED | PA79 | Vehicle Speed Signal
80 | GRN | U80 | Tachometer Output
81 | -- | -- | NOT USED
82 | BRN/YEL | XB82 | TPS Signal Output
83 | GRY | R83 | Delivered Engine Torque Output
84-87 | -- | -- | NOT USED
88 | BRN/WHT | XM88 | Serial Data

#### Engine Controls Power Relay K43

Connector Part Information | ZF 9-31
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | -- | -- | NOT USED
2 | RED | A71, A73 | B+ from fuse V5
3 | -- | -- | NOT USED
4 | RED | A73 | B+ from fuse V5
5 | -- | -- | NOT USED
6 | BRN/GRY | XR46 | Relay K43 control
7 | -- | -- | NOT USED
8 | RED/BLU | AP75 | Switched B+ from relay K43
9 | -- | -- | NOT USED

#### Engine Coolant Temperature (ECT) Sensor

Connector Part Information | ZFW 2-83
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BRN/BLU | XP74 | ECT sensor ground
2 | BRN/GRN | XU715 | Sensor ground

#### Engine Oil Level Sensor

Connector Part Information | ZFW 2-31
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BLK | F120 | Ground to G103
2 | BRN/GRN | XU4 | Low oil level signal

#### Evaporative (EVAP) Purge Solenoid Valve

Connector Part Information | AM 962069
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP108 | B+ from relay K43
2 | BRN/RED | XA61 | EVAP purge solenoid valve control

#### Evaporative (EVAP) Tank Solenoid Valve

Connector Part Information | AM 962069
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP115 | B+ from fuel injection relay
2 | BRN/BLK | XF65 | EVAP tank solenoid valve control

#### Fuel Injector #1

Connector Part Information | ZFW 2-44
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP61 | B+ from relay K43
2 | BRN/BLK | XB17 | Fuel injector #1 control

#### Fuel Injector #2

Connector Part Information | ZFW 2-44
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP63 | B+ from relay K43
2 | BRN/PPL | XU16 | Fuel injector #2 control

#### Fuel Injector #3

Connector Part Information | ZFW 2-44
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP64 | B+ from relay K43
2 | BRN/BLU | XP35 | Fuel injector #3 control

#### Fuel Injector #4

Connector Part Information | ZFW 2-44
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP62 | B+ from relay K43
2 | BRN/RED | XA34 | Fuel injector #4 control

#### Fuel Injector #5

Connector Part Information | ZFW 2-44
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP65 | B+ from relay K43
2 | BRN/RED | XF15 | Fuel injector #5 control

#### Fuel Injector #6

Connector Part Information | ZFW 2-44
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP66 | B+ from relay K43
2 | BRN/GRN | XY33 | Fuel injector #6 control

#### Fuel Pump

Connector Part Information | ZFW 5-3
--- | ---
Pin | Wire Color | Circuit No. | Function
A | RED/BLU | AP10 | B+ from fuse #18
B | BLK | F224 | Ground to G103
C | BLK | F30 | Ground to G400
D | BLU/BLK | PF11 | Low fuel level signal

#### Fuel Pump Relay K44

Connector Part Information | ZF 9-31
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | -- | -- | NOT USED
2 | RED | A72 | B+ from fuse V5
3 | -- | -- | NOT USED
4 | RED/BLU | AP76 | B+ from relay K43
5 | -- | -- | NOT USED
6 | BRN/BLU | XR3 | Relay control signal
7 | -- | -- | NOT USED
8 | RED/BLU | AP77 | B+ feed to fuse #18
9 | -- | -- | NOT USED

#### Fuel Tank Pressure Sensor

Connector Part Information | ZFW 3-20
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BLU/BLK | PF1 | 5V reference
2 | BRN/GRN | XU1 | Sensor ground
3 | BRN/YEL | XB1 | Fuel pressure sensor signal

#### Heated Oxygen Sensor (Bank 1, Position 1)

Connector Part Information | ZFW 4-2
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP122 | B+ from fuse #39
2 | BRN/WHT | XM301 | HO2S heater control
3 | BRN/BLU | XU462 | HO2S ground
4 | BRN/BLU | XP19 | HO2S signal

#### Heated Oxygen Sensor (Bank 2, Position 1)

Connector Part Information | ZFW 4-2
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP124 | B+ from fuse #39
2 | BRN/WHT | XM302 | HO2S heater control
3 | BRN/GRN | XU464 | HO2S ground
4 | BRN/BLU | XP18 | HO2S signal

#### Heated Oxygen Sensor (Bank 2, Position 2)

Connector Part Information | ZFW 4-2
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP123 | B+ from fuse #39
2 | BRN/WHT | XM122 | HO2S heater control
3 | BRN/GRN | XU463 | HO2S ground
4 | BRN/BLU | XP76 | HO2S signal

#### Heated Oxygen Sensor (Bank 1, Position 2)

Connector Part Information | ZFW 4-2
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP121 | B+ from fuse #39
2 | BRN/WHT | XM111 | HO2S heater control
3 | BRN/GRN | XU461 | HO2S Ground
4 | BRN/BLU | XP77 | HO2S signal

#### Idle Air Control (IAC) Valve

Connector Part Information | ZFW 3-23
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BRN/BLU | XP2 | Valve closed signal control
2 | RED/BLU | AP101 | Switched positive battery voltage
3 | BRN/RED | XA29 | Valve open signal

#### Ignition Coil

Connector Part Information | ZFW 4-5
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BLK/YEL | FB20 | 2-5 ignition control
2 | BLK/RED | FA21 | 6-3 ignition control
3 | GRY/BLK | FR1 | 1-4 ignition control
4 | BRN | X68 | B+ from ignition switch

#### Intake Air Temperature (IAT) Sensor

Connector Part Information | ZFW 2-40
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BLU/RED | PA16 | IAT sensor signal
2 | BRN/GRN | XU714 | Sensor ground

#### Intake Plenum Switch-Over Solenoid Valve

Connector Part Information | ZFW 2-40
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BRN/GRN | XU35 | B+ from relay K43
2 | RED/BLU | AP105 | Intake plenum switch-over solenoid valve control

#### Intake Resonance Switch-Over Valve Solenoid Valve

Connector Part Information | ZFW 2-40
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BRN/GRN | XU7 | B+ from relay K43
2 | RED/BLU | AP104 | Intake resonance switch-over solenoid valve control

#### Knock Sensor (Bank 1)

Connector Part Information | ZFW 2-83
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BRN/WHT | XM70 | KS bank 1 signal
2 | BRN/BLK | XF420 | KS ground

#### Knock Sensor (Bank 2)

Connector Part Information | ZFW 2-83
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BRN/WHT | XM40 | KS bank 2 signal
2 | BRN/BLK | XF410 | KS ground

#### Mass Air Flow (MAF) Sensor

Connector Part Information | ZFW 4-7
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BLK | F81 | Ground to G102
2 | BRN/GRN | XU306 | Sensor ground
3 | RED/BLU | AP84 | B+ from relay K43
4 | BLU/GRN | PU7 | MAF sensor signal

#### Secondary Air Injection Pump

Connector Part Information | ZFW 2-24
--- | ---
Pin | Wire Color | Circuit No. | Function
A | PPL | Y110 | Pump ON signal
B | BLK | F110 | Ground to G103

#### Secondary Air Injection Pump Relay K12

Connector Part Information | ZF 9-32
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | -- | -- | NOT USED
2 | PPL | Y110 | Pump ON signal
3 | -- | -- | NOT USED
4 | RED/BLU | AP200, AP900 | B+ from relay K43
5 | BLK | F200 | Ground to G103
6 | BRN/GRY | XR200 | Relay control signal
7 | -- | -- | NOT USED
8 | RED | AP730 | B+ from fuse #49
9 | -- | -- | NOT USED

#### Secondary Air Injection Pump Solenoid Valve

Connector Part Information | ZFW 2-35
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | RED/BLU | AP900 | B+ from relay K43
2 | BRN/YEL | XB900 | Solenoid valve control signal

#### Throttle Position Sensor

Connector Part Information | ZFW3-23
--- | ---
Pin | Wire Color | Circuit No. | Function
1 | BRN/GRN | XU305 | Sensor ground
2 | BLU/BLK | PF533 | 5V reference
3 | BRN/BLU | XP53 | TP sensor signal