For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Master Cylinder Pushrod Clevis Pin Bore to Top of Booster Housing | 180 mm | 7.1 in
Brake Master Cylinder Pushrod Clevis Pin Bore to Top of Support Bracket Dimension | 106 mm | 4.2 in
Brake Pedal Travel

- Maximum Specification with 445 N (100 lbs) of force applied to the brake pedal with the igntion OFF and the booster power reserve depleted

72 mm

2.84 in