For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Instrument Cluster System Check performed? | -- | Go to Step 2 | Go to Instrument Cluster System Check
2 | Is the warning lamp inoperative? | -- | Go to Step 3 | Go to Step 4
3 |

1. Install the scan tool.
2. Select SPECIAL FUNCTIONS from the INSTRUMENT CLUSTER menu.
3. Command the Low Fuel Lamp ON and OFF.

Does the lamp respond when commanded?

--

Go to Instrument Cluster System Check

Go to Step 5

4 | Is the warning lamp ON at all times? | -- | Go to Step 6 | Go to Step 5
5 | Replace and program the instrument cluster. For the replacement procedure. Refer to Instrument Panel, Gauges and Console Is the replacement complete? | -- | Go to Instrument Cluster System Check | --
6 |

1. Install the scan tool.
2. Select SPECIAL FUNCTIONS from the INSTRUMENT CLUSTER menu.
3. Command the Low Fuel Lamp OFF.

Does the lamp respond when commanded?

--

Go to Instrument Cluster System Check

Go to Step 5