For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Body Control Module (BCM) | Mounted on the right A-Pillar, behind the trim panel | Body Control System Component Views in Body Control System | Body Control System Connector End Views in Body Control System
Data Link Connector (DLC) | Attached to the IP carrier, to the left of the steering column | -- | Data Link Communications Connector End Views in Data Link Communications
Electronic Brake/Traction Control Module (EBTCM) | Left front of the engine compartment, mounted to the lower rail | Antilock Brake System Component Views in Antilock Brake System | Antilock Brake System Connector End Views in Antilock Brake System
Engine Control Module (ECM) | Left front of the engine compartment, in the ECM housing, at position 40 | Engine Controls Component Views in Engine Controls - 3.0L | Engine Controls Connector End Views in Engine Controls - 3.0L
Front Side Door Jamb Switch (LH) | Lower left A-Pillar | -- | Lighting Systems Connector End Views in Lighting Systems
Front Side Door Jamb Switch (RH) | Lower right A-Pillar | -- | Lighting Systems Connector End Views in Lighting Systems
Front Side Door Lock Switch (LH) | Mounted to the inside left front side door trim panel | -- | Lighting Systems Connector End Views in Lighting Systems
Front Side Door Lock Switch (RH) | Mounted to the inside right front side door trim panel | -- | Lighting Systems Connector End Views in Lighting Systems
Fuse Block | Mounted to the IP, lower left side of the steering column | -- | --
Gauge Cluster | Left side of the IP, just to the left and above the heater & A/C control | -- | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges and Console
Horn Relay K63 | Lower IP, to the right side of the steering column, on the relay box | -- | Horn Connector End Views in Horns
Ignition Switch | Mounted to the ignition lock cylinder | -- | Engine Electrical Connector End Views in Engine Electrical
Low Beam Relay K131 | Lower IP, to the right side of the steering column, on the relay box | Power and Grounding Component Views in Wiring Systems | Lighting Systems Connector End Views in Lighting Systems
Park Lamp Relay K130 | Lower IP, to the right side of the steering column, on the relay box | Power and Grounding Component Views in Wiring Systems | Lighting Systems Connector End Views in Lighting Systems
Power Distribution Fuse Block | Left side of the engine compartment, attached to the ECM housing, above the battery | Power and Grounding Component Views in Wiring Systems | --
Rear Compartment Courtesy Lamp Switch | Attached to the rear compartment lid | -- | --
Rear Side Door Jamb Switch (LH) | Lower left B-Pillar | -- | Lighting Systems Connector End Views in Lighting Systems
Rear Side Door Jamb Switch (RH) | Lower right B-Pillar | -- | Lighting Systems Connector End Views in Lighting Systems
Theft Deterrent Module | Mounted to the ignition lock cylinder, on the upper right side of the steering column | -- | Theft Deterrent System Connector End Views
C200A | IP wiring harness to body wiring harness, at the lower left A-Pillar | Power and Grounding Component Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200B | IP wiring harness to body wiring harness, at the lower left A-Pillar | Power and Grounding Component Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C301 | Body wiring harness to right courtesy lamp wiring harness, at the base of the right B-Pillar | -- | Inline Harness Connector End Views in Wiring Systems
C302 | Body wiring harness to left courtesy lamp wiring harness, at the base of the left B-Pillar | -- | Inline Harness Connector End Views in Wiring Systems
C405 | Body wiring harness to rear compartment lid harness | -- | Inline Harness Connector End Views in Wiring Systems
C500 | Body wiring harness to left front side door wiring harness, at the lower left A-Pillar, near G200 | Power Door Systems Component Views in Doors | Inline Harness Connector End Views in Wiring Systems
C600 | Body wiring harness to right front side door wiring harness, at the lower right A-Pillar | Power Door Systems Component Views in Doors | Inline Harness Connector End Views in Wiring Systems
G103 | Body and IP wiring harnesses, located at the left front of the engine compartment, near C102, C105, and C106, underneath the battery tray | Wiper/Washer Component Views in Wiper/Washer System | --
G200 | Body wiring harness, at the lower left A-Pillar, above and to the right of C200 | Power and Grounding Component Views in Wiring Systems | --
P103 | Lower left A-Pillar, forward of G200 | Power and Grounding Component Views in Wiring Systems | --
P108 | Left engine compartment, at the rear of the ECM housing | -- | --
P110 | Rear left corner of the engine compartment | -- | --
P401 | Lower left corner of the rear compartment | -- | --
P402 | Upper left corner of the rear compartment, near the left taillamp | -- | --
P500 | In the left front side door, approximately 12 cm (5 in) from the outside remote control rear view mirror switch | -- | --
P600 | In the right front side door, approximately 25 cm (10 in) from the right front side door lock switch | -- | --
S103 | Body wiring harness, approximately 15 cm (6 in) from branch break off for the left headlamp, towards the EBTCM branch break off | -- | --
S104 | Body wiring harness, approximately 71 cm (28 in) from P103, towards the EBTCM branch break off | -- | --
S200 | IP wiring harness, approximately 15 cm (6 in) from cruise release switch and stoplamp switch branch break off, towards G201 branch break off | -- | --
S214 | IP wiring harness, approximately 17 cm (7 in) from cruise release switch and stoplamp switch branch break off, towards G201 branch break off | -- | --
S222 | IP wiring harness, near G201 branch break off | -- | --
S245 | IP wiring harness, near the multifunction relay module connector branch break off | -- | --
S250 | IP wiring harness, near the instrument cluster connector branch break off | -- | --
S251 | IP wiring harness, near the G201 branch break off | -- | --
S267 | Body wiring harness, near G200 branch break off | -- | --
S270 | Body wiring harness, approximately 70 cm (27 in) from the console wiring branch break off | -- | --
S308 | Body wiring harness, base of the right A-Pillar, just under the conduit | -- | --
S309 | Body wiring harness, base of the right A-Pillar, just under the conduit | -- | --
S312 | Body wiring harness, base of the left A-Pillar, just under the conduit | -- | --
S314 | Body wiring harness, base of the left A-Pillar, just under the conduit | -- | --
S317 | Body wiring harness, base of the left A-Pillar, just under the conduit | -- | --
S319 | Body wiring harness, base of the left A-Pillar, just under the conduit | -- | --
S502 | Left front side door wiring harness, approximately 26 cm (10 in) from connector | -- | --
S602 | Left front side door wiring harness, approximately 26 cm (10 in) from connector | -- | --