For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Driver Seat Belt Side Buckle Pretensioner | Mounted to the lower RH side of the driver's seat | Seat Belt Component View | --
Passenger Seat Belt Side Buckle Pretensioner | Mounted to the lower LH side of the passenger's seat | Seat Belt Component View | --
Seat Belt Switch | Part of the driver's seat belt buckle | -- | --
C200B | I/P wiring harness to body wiring harness, at lower LH A-pillar | Power and Grounding Component Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C315 | Body wiring harness to driver's seat, underneath the driver's | -- | Seat Belt Connector End Views in Seat Belts
C315B | Seat belt switch to body wiring harness, underneath the driver's seat | Seat Belt Component View | --
G103 | Body and I/P wiring harnesses, located at the LH front of the engine compartment, near C102, C105 and C106 | Wiper/Washer Component Views in Wiper/Washer System | --
P103 | Lower LH A-pillar, forward of G200 | Power and Grounding Component Views in Wiring Systems | --
P110 | Rear LH corner of the engine compartment | -- | --
S104 | Body wiring harness, approximately 83 cm (32 in) from P103, near P107 | -- | --
S103 | Body wiring harness, approximately 27 cm (10 in) from P107 | -- | --
S106 | A/C control wiring harness, approximately 12 cm (5 in) from the C111 branch break off | -- | --
S251 | I/P wiring harness, near the G201 branch break off | -- | --