For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Automatic Transmission Range Switch | LH side of the transmission housing | Automatic Transmission Electronic Component Views in Automatic Transmission | Lighting Systems Connector End Views in Lighting Systems
Fuse Block | Mounted to the I/P, lower LH side of the steering column | -- | --
Heated Outside Rear View Mirror and Rear Window Defogger Relay K35 | Lower I/P, to the RH side of the steering column, on the relay box (roman numeral III) | -- | Stationary Windows Connector End Views
Heater and A/C Control | Center of the I/P, above the radio | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | HVAC Connector End Views in HVAC Systems
Ignition Switch | Mounted on the upper RH side of the steering column | -- | Engine Electrical Connector End Views in Engine Electrical
Inside Rear View Mirror | Attached to the upper center of the windshield | Power Roof Systems Component Views in Roof | Stationary Windows Connector End Views
Multifunction Relay K134 | Under the LH side of the I/P | Power and Grounding Component Views in Wiring Systems | Lighting Systems Connector End Views in Lighting Systems
Outside Rear View Mirror (LH) | Attached to the LH front side door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Outside Rear View Mirror (RH) | Attached to the RH front side door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Radio Antenna Amplifier | On top of the rear deck, under the trim panel | -- | --
Radio, AM/FM Stereo and Clock and Tape Player and Compact Disk Player | Center of the I/P, below the heater and A/C control | -- | Entertainment Connector End Views in Entertainment
Rear Window Defogger Grid | Mounted on the rear window | -- | --
C105 (green connector) | I/P wiring harness to ECM wiring harness, in the LH front of the engine compartment, just behind battery | Wiper/Washer Component Views in Wiper/Washer System | Inline Harness Connector End Views in Wiring Systems
C106 (blue connector) | I/P wiring harness to ECM wiring harness, in the LH front of the engine compartment, just behind battery | Wiper/Washer Component Views in Wiper/Washer System | Inline Harness Connector End Views in Wiring Systems
C200A | I/P wiring harness to body wiring harness, at lower LH A-pillar | Power and Grounding Component Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C202 | I/P wiring harness to rear amplifier wiring harness, at lower RH A-pillar, next to BCM | -- | --
C500 | Body wiring harness to the LH front side door wiring harness, at lower LH A-pillar, near G200 | Power Door Systems Component Views in Doors | Inline Harness Connector End Views in Wiring Systems
C600 | Body wiring harness to the RH front side door wiring harness, at lower RH A-pillar | Power Door Systems Component Views in Doors | Inline Harness Connector End Views in Wiring Systems
G103 | Body and I/P wiring harness, located at the LH front of the engine compartment, underneath the battery tray | Wiper/Washer Component Views in Wiper/Washer System | --
G200 | Body wiring harness, at the lower LH A-pillar, mounted above C200 | -- | --
G400 | Body wiring harness, in the lower LH corner of the rear compartment, near the LH stop/taillamp | -- | --
P103 | Lower LH A-pillar, forward of G200 | Power and Grounding Component Views in Wiring Systems | --
P110 | Rear LH corner of the engine compartment | -- | --
S103 | Body wiring harness, approximately 15 cm (6 in) from branch break off for the LH headlamp, towards the EBTCM branch break off | -- | --
S132 | ECM wiring harness, inside the ECM housing, approximately 10 cm (4 in) from P108 | -- | --
S140 | I/P wiring harness, near the brake fluid minimum capacity sensor connector branch break off | -- | --
S200 | I/P wiring harness, approximately 15 cm (6 in) from cruise release switch and stoplamp switch branch break off, towards G201 branch break off | -- | --
S214 | I/P wiring harness, approximately 17 cm (7 in) from cruise release switch and stoplamp switch branch break off, towards G201 branch break off | -- | --
S220 | I/P wiring harness, near the DLC branch break off | -- | --
S251 | I/P wiring harness, near the G201 branch break off | -- | --
S252 | I/P wiring harness, near the G201 branch break off | -- | --
S270 | Body wiring harness, approximately 62 cm (25 in) from the C200 branch break off, toward the driver's side | -- | --
S308 | Body wiring harness, base of RH A-pillar, just under conduit | -- | --
S326 | Body wiring harness, base of LH A-pillar, just under conduit | -- | --
S502 | LH front side door wiring harness, approximately 26 cm (10 in) from the C500 branch break off | -- | --
S602 | RH front side door wiring harness, approximately 26 cm (10 in) from the C600 branch break off | -- | --