For 1990-2009 cars

#### Central Locking Relay (K135)

Connector Part Information |

• | F 14-3

• | 14-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/RED | FA811 | Fuel Door Release Relay Control
BRN/PPL | XY804 | Fuel Door Release Relay Control
2 | BLK/RED | FA809 | Driver Door Lock Actuator UNLOCK Control
3 | -- | -- | Not Used
4 | BRN/PPL | XY803 | Drivers Door UNLOCK Control
5 | RED | A888 | Battery Positive Voltage
6 | BLK/RED | FA805 | Fuel Door Release Actuator Supply Voltage
7 | BRN/PPL | XY807 | Door UNLOCK Control
8 | RED | A911 | Battery Positive Voltage
9 | BLK/RED | FA812 | Rear Compartment Lid Release Relay Control
BRN/PPL | XY805 | Rear Compartment Lid Release Relay Control
10 | BLK/RED | FA801 | Door Lock Actuator UNLOCK Control
11 | BRN/PPL | XY806 | Door Lock Control
12 | BLK/YEL | FB801 | Door Lock Actuator LOCK Supply Voltage
13 | BLK/RED | FA807 | Rear Compartment Lid Release Actuator Supply Voltage
14 | BLK | F911 | Ground

#### Door Lock Actuator - Driver

Connector Part Information |

• | ZFW 6-6

• | 6-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BLK/RED | FA809 | Drivers Door Lock Actuator UNLOCK Control
3-5 | -- | -- | Not Used
6 | BLK/YEL | FB9 | Door Lock Actuator Lock Control

#### Door Lock Actuator - LR

Connector Part Information |

• | ZFW 6-6

• | 6-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BLK/RED | FA804 | Door Lock Actuator UNLOCK Control
3-5 | -- | -- | Not Used
6 | BLK/YEL | FB805 | Door Lock Actuator LOCK Control

#### Door Lock Actuator - Passenger Front

Connector Part Information |

• | ZFW 6-6

• | 6-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BLK/RED | FA809 | Door Lock Actuator UNLOCK Control
3-5 | -- | -- | Not Used
6 | BLK/YEL | FB9 | Door Lock Actuator LOCK Control

#### Door Lock Actuator - RR

Connector Part Information |

• | ZFW 6-6

• | 6-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BLK/RED | FA804 | Door Lock Actuator UNLOCK Control
3-5 | -- | -- | Not Used
6 | BLK/YEL | FB805 | Door Lock Actuator LOCK Control

#### Door Switch - Driver

Connector Part Information |

• | ZF32-1

• | 32-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-3 | -- | -- | Not Used
4 | RED | A21 | Battery Positive Voltagel
5 | WHT | M5 | Power Window Master Switch LOCKOUT Signal
6 | BLK | F30 | Ground
7 | BLU/RED | PA4 | Power Window Master Switch Right Rear DOWN Signal
8 | GRY/GRN | RU15 | Power Window Master Switch Right Rear UP Signal
9 | BLU/RED | PA1 | PowerWindow Master Switch Right Front DOWN Signal
10 | GRY/GRN | RU1 | Power Window Master Switch Right Front UP Signal
11 | BRN | X10 | Battery Positive Voltage
12 | BLK/RED | FA2 | Mirror Motor Control
13 | YEL | B10 (w/AG8) B2 (w/o AG8) | Driver Mirror Motor UP/DOWN Signal
14 | GRY | R11 | Passenger Mirror Motor UP/DOWN Signal
15 | GRN | U10 (w/AG8) U1 (w/o AG8) | Driver Mirror Motor RIGHT/LEFT Signal
16 | BLU | P3 | Passenger Mirror Motor RIGHT/LEFT Signal
17-19 | -- | -- | Not Used
20 | GRY | R10 | Secondary Door Latch Switch Signal
21 | GRY/WHT | RM10 | Driver Door Open Signal
22 | GRY/YEL | RB50 | Park Lamp Switch On Input/Park Lamp Relay Control
23 | BLU/RED | PA3 | Power Window Master Switch Left Rear DOWN Signal
24 | GRY/GRN | RU15 | Power Window Master Switch Left Rear UP Signal
25 | BLU/RED | PA2 | Power Window Motor Left Front DOWN Signal
26 | GRY/GRN | RU6 | Power Window Motor Left Front UP Signal
27 | GRY/YEL | RB43 | Instrument Panel Lamp Supply Voltage-1
28 | GRY/YEL | RB42 | Instrument Panel Lamp Supply Voltage-1
29 | YEL | B6 | Power Window Switch EXPRESS Signal
30 | -- | -- | Not Used
31 | BLK/BRN | FX805 | Driver Door Lock Switch LOCK Signal
32 | BLK/BRN | FY805 | Driver Door Lock Switch UNLOCK Signal

#### Door Switch - Front Passenger

Connector Part Information |

• | F 4-17

• | 8-Way F (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLU/RED | PA22 | Power Window Motor Right Front DOWN Control
2 | GRY/GRN | RU22 | Power Window Motor Right Front UP Control
3 | YEL | B6 | Power Window Switch EXPRESS Signal
4 | GRY/YEL | RB43 | Instrument Panel Lamp Supply Voltage-1
5 | BLK | F20 | Ground
6 | BLK/BRN | FX805 | Driver Door Lock Switch LOCK Signal
7 | BLK/PPL | FY805 | Driver Door Lock Switch UNLOCK Signal
8 | -- | -- | Not Used

#### Outside Rearview Mirror - Driver (w/AG8)

Connector Part Information |

• | ZF 9-21

• | 9-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YEL | B20 | Driver Mirror Motor DOWN Control
2 | GRN | U200 | Driver Mirror Motor RIGHT Control
3 | BLK/RED | FA81 | Mirror MOTOR Control
4 | RED | X60 | 5-Volt Reference
5 | BLK/BRN | FX60 | Low Reference
6 | GRY | R60 | Driver Mirror VERTICAL POSITION Sensor Signal
7 | GRY/GRN | RU60 | Driver Mirror HORIZONTAL POSITION Sensor Signal
8 | BLK/WHT | FM15 | Heated Mirror Element SUPPLY Voltage
9 | BLK | F50 | Ground

#### Outside Rearview Mirror - Driver (w/o AG8)

Connector Part Information |

• | ZF 9-21

• | 9-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YEL | B2 | Driver Mirror Motor DOWN Control
2 | GRN | U1 | Driver Mirror Motor RIGHT Control
3 | BLK/RED | FA2 | Mirror MOTOR Control
4-7 | -- | -- | Not Used
8 | BLK/WHT | FM2 | Heated Mirror Element SUPPLY Voltage
9 | BLK | F2 | Ground

#### Outside Rearview Mirror - Passenger (w/AG8)

Connector Part Information |

• | ZF 9-21

• | 9-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY | R5 | Passenger Mirror Motor DOWN Control
2 | BLU | P10 | Passenger Mirror Motor RIGHT Control
3 | BLK/RED | FA65 | Mirror MOTOR Control
4 | BRN | X65 | 5-Volt Reference
5 | BLK/BRN | FX65 | Low Reference
6 | GRY | R70 | Passenger Mirror VERTICAL Position Sensor Signal
7 | GRY/GRN | RU60 | Passenger Mirror HORIZONTAL Position Sensor Signal
8 | BLK/WHT | FM20 | Heated Mirror Element SUPPLY Voltage
9 | BLK | F55 | Ground

#### Outside Rearview Mirror - Passenger (w/o AG8)

Connector Part Information |

• | ZF 9-21

• | 9-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY | R4 | Passenger Mirror Motor DOWN Control
2 | BLU | P2 | Passenger Mirror Motor RIGHT Control
3 | BLK/RED | FA4 | Mirror MOTOR Control
4-7 | -- | -- | Not Used
8 | BLK/WHT | FM2 | Heated Mirror Element SUPPLY Voltage
9 | BLK | F2 | Ground

#### Window Motor - Driver

Connector Part Information |

• | ZFW 6-6

• | 6-Way F (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RED | A20 | Battery Positive Voltage
2 | GRY/GRN | RU6 | Power Window Motor Left Front UP Signal
3 | BLU/RED | PA2 | Power Window Motor Left Front DOWN Signal
4 | BLK | F11 | Ground
5 | YEL | B11 | Power Window Switch EXPRESS Signal
6 | -- | -- | Not Used

#### Window Motor - Front Passenger

Connector Part Information |

• | ZFW 6-6

• | 6-Way F (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RED | A2 | Battery Positive Voltage
2 | GRY/GRN | RU6 | PowerWindow Master Switch Right Front UP Signal
3 | BLU/RED | PA2 | Power Window Master Switch Right Front DOWN Signal
4 | BLK | F11 | Ground
5 | YEL | B2 | Power Window Switch EXPRESS Signal
6 | -- | -- | Not Used

#### Window Motor - LR

Connector Part Information |

• | ZFW 6-6

• | 6-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RED | A1 | Battery Positive Voltage
2 | GRY/GRN | RU2 | Power Window Master Switch Left Rear UP Signal
3 | BLK/RED | PA2 | Power Window Master Switch Left Rear DOWN Signal
4 | BLK | F1 | Ground
5 | YEL | B1 | Power Window Switch EXPRESS Signal
6 | -- | -- | Not Used

#### Window Motor - RR

Connector Part Information |

• | ZFW 6-6

• | 6-Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RED | A1 | Battery Positive Voltage
2 | GRY/GRN | RU2 | Power Window Master Switch Right Rear UP Signal
3 | BLK/RED | PA2 | Power Window Master Switch Right Rear DOWN Signal
4 | BLK | F1 | Ground
5 | YEL | B1 | Power Window Switch EXPRESS Signal
6 | -- | -- | Not Used

#### Window Switch - LR

Connector Part Information |

• | ZF 5-9

• | 5-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLU/RED | PA1 | Power Window Motor Left Rear DOWN Control
B | GRY/GRN | RU1 | Power Window Motor Left Rear UP Control
C | WHT | M1 | Power Window Master Switch LOCKOUT Signal
D | GRY/YEL | RB42 | Instrument Panel Lamp SUPPLY Voltage-1
E | BLK | F2 | Ground

#### Window Switch - RR

Connector Part Information |

• | ZF 9-5

• | 5-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLU/RED | PA1 | Power Window Motor Right Rear DOWN Control
B | GRY/GRN | RU1 | Power Window Motor Right Rear UP Control
C | WHT | M1 | Power Window Master Switch LOCKOUT Signal
D | GRY/YEL | RB42 | Instrument Panel Lamp SUPPLY Voltage-1
E | BLK | F2 | Ground