For 1990-2009 cars

#### Automatic Transmission Range Switch

Connector Part Information |

• | ZPF 8-3

• | 8 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/BLU | FP723 | Transmission Position Signal
B | BLK/GRN | FU726 | Transmission Position Signal
C | BLK/YEL | FB708 | Transmission Position Signal
D | BRN | X756 | B+ from Fuse #3
E | BLK/RED | FA501 | Starter Solenoid Signal
F | WHT/BLK | MF757 | Rear View Mirror/Backup Lamp Feed
G | GRY | R733 | Transmission Position Signal
H | BLK/RED | FA500 | B+ in the ON Position

#### Auxiliary Brake Lamp

Connector Part Information |

• | ZPM 2-50

• | 2 Way M

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | F3 | Ground to G400
B | BLK/YEL | FB5 | Lamp ON Signal

#### Daytime Running Lamps Relay K133

Connector Part Information |

• | ZFW 5-20

• | 5 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN/PPL | XY802 | Relay Control
2 | -- | -- | Not Used
3 | RED | A825 | B+ from Fuse #21
4 | WHT | M8 | Lamp ON Signal
5 | RED | A10 | B+ from Fuse #21

#### Dome and Reading Lamps

Connector Part Information |

• | BLKF 4-21

• | 4 Way F

• | BLK

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN/BLU | XP806 | Ground from Relay K134
2 | BLK | F901 | Ground to G103
3 | RED/BLU | AP882 | B+ from Relay K134
4 | RED/BLU | AP808 | B+ from Relay K134

#### Hazard Warning Switch

Connector Part Information |

• | ZF 9-4

• | 9 Way F

• | BLK

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/WHT | FM22 | Hazard Signal
2 | BLK | F27 | Ground to G103
3 | BLU | P3 | Ignition Positive Voltage
4 | BLK/WHT | FM3 | LH Hazard ON Signal
5 | -- | -- | Not Used
6 | RED | A9 | B+ from Fuse #12
7 | BLK/GRN | FU3 | RH Hazard ON Signal
8 | GRY/YEL | RB77 RB70 | Dimmer Output Signal
9 | BRN | X10 | B+ from Fuse #3

#### Headlamp Automatic Control Ambient Light Sensor

Connector Part Information |

• | F4-21

• | 4 Way F

• | BLK

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN | X812 | 5 V Reference
2 | BLK/WHT | FM60 | Sun Sensor Input Signal
3 | BLK | F830 | Day/Night Signal
4 | BLU | P111 | Sensor Ground

#### Headlamp Switch

Connector Part Information |

• | ZF 18-7

• | 18 Way F

• | GRY

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY/GRN | RU70 | B+ from Fuse #26
2 | GRY/YEL | RB1 | Dimmer Output Signal
3 | BRN | X22 | B+ from Fuse #15
4 | BRN/RED | XA811 | Low Beam Relay Signal
5 | BRN/WHT | XM815 | Park Lamp Relay Signal
6 | YEL | B60 | Low Beam ON/OFF Signal
7 | RED/WHT | AM813 | Park Lamp ON/OFF Signal
8 | BRN/PPL | XY112 | Interior lamps ON/OFF signal
9 | RED/YEL | AB810 | TS ON/OFF Signal
10 | BLK/BLU | FP28 | Fog Lamp Switch Signal
11 | BLK/BRN | FX810 | TS Delay Signal
12 | BLK/PPL | FY810 | TS Return Signal
13 | BLK | F18 | Ground to G103
14 | YEL | B55 | B+ form Fuse #22
15 | -- | -- | Not Used
16 | BRN/BLK | XF830 | TS Indicator
17 | RED | A5 | B+ from Fuse #8
18 | GRY/WHT | RM901 | Chime Control Signal

#### I/P Compartment Lamp

Connector Part Information |

• | F 2-14

• | 2 Way F

• | BLK

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED/BLU | AP802 | B+ from Multifunction Relay
B | BLK | F72 | Lamp ON Signal Relay

#### I/P Compartment Lamp Switch

Connector Part Information |

• | F 2-14

• | 2 Way F

• | BLK

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | F71 | Ground to G103
B | BLK | F72 | Lamp ON Signal

#### LH Backup Lamp

Connector Part Information |

• | PF 2-1

• | 2 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK | F1 | Ground to G400
2 | WHT/BLK | MF10 MF1 | Lamp ON Feed

#### LH Cornering Lamp

Connector Part Information |

• | ZFW 2-9

• | 2 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY/BLK | RF1 | Lamp ON Signal
2 | BLK | F2 | Ground to G103

#### LH Fog Lamp

Connector Part Information |

• | ZFW 2-10

• | 2 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/BLU | FP2 | Lamp ON Signal
2 | BLK | F3 | Ground to G103

#### LH Front Side Door Jamb Switch

Connector Part Information |

• | F 2-42

• | 2 Way F

• | BLK

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY/WHT | RM2 | Door Open Signal
2 | GRY | R2 | Door Open Signal

#### LH Front Side Door Lock Switch

Connector Part Information |

• | F 4-21

• | 4 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/BRN | FX805 | Door Lock Signal
2 | BLK/PPL | FY805 | Door Unlock Signal
3 | RED/BLU | AP807 | Illumination Signal
4 | BLK | F12 | Ground to G200

#### LH Front Side Marker Lamp

Connector Part Information |

• | ZFW 2-9

• | 2 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/WHT | FM1 | Ground
2 | GRY/GRN | RU2 | Lamp ON Signal

#### LH Headlamp Relay (High Beam) K73

Connector Part Information |

• | ZFW 5-20

• | 5 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WHT | M70 | Relay Control
2 | WHT | M65 | Lamp ON Signal
3 | RED | A832 | B+ from Fuse #21
4 | BLK | F803 | Ground to G103
5 | BLK/WHT | FM19 | Lamp ON Signal

#### LH Headlamp

Connector Part Information |

• | ZPF 5-1

• | 5 Way F

• | BLK

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | BLK/WHT | FM13 | High Beam Signal
C | YEL | B1 | Low Beam Signal
D | BLK | F840 | Ground to G103
E | WHT | M2 | High Beam Signal

#### LH Park/Turn Signal Lamp

Connector Part Information |

• | ZFW 3-21

• | 3 Way F

• | GRY

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | F12 | Ground to G103
B | GRY/BLK | RF3 | Park Lamp Signal
C | BLK/WHT | FM2 | Park Lamp Signal

#### LH Rear Side Door Jamb Switch

Connector Part Information |

• | F 2-42

• | 2 Way F

• | BLK

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY | R2 | Door Open Signal
2 | GRY | R1 | Door Open Signal

#### LH Rear Side Marker Lamp

Connector Part Information |

• | ZFW 2-9

• | 2 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY/BLK | RF1 | Lamp ON Signal
2 | BLK/WHT | FM1 | Ground

#### LH Stop/Taillamp

Connector Part Information |

• | PF 4-2

• | 4 Way F

• | BLK

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/YEL | FB6 | Brake Lamp Signal
B | GRY/BLK | RF4 | Lamp ON Signal
C | BLK | F125 | Ground to G400
D | BLK/WHT | FM20 | Lamp ON Signal

#### LH Sunshade Illuminated Mirror Lamp

Connector Part Information |

• | ZPF 2-50

• | 2 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | F3 | Ground to G103
B | RED/BLU | AP3 | B+ from Multifunction Relay

#### Low Beam Relay K131

Connector Part Information |

• | ZFW 5-20

• | 5 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN/RED | XA810 XA811 | Relay Control
2 | -- | -- | Not Used
3 | RED/WHT | AM811 | Exterior Lamp Power
4 | YEL | B50 | Lamps ON Signal
5 | RED | A814 | B+ from Fuse V3

#### Multifunction Relay K134

Connector Part Information |

• | F 14-3

• | 14 Way F

• | BLK

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/RED | FA888 | High Beam ON Signal
2 | RED/BLU | AP805 | Rear Compartment Open Signal
3 | GRY/BLK | RF75 | B+ from Fuse #26
4 | BLK/BLU | FP36 | Fog Lamp Indicator Signal
5 | RED | A831 | B+ from Fuse #29
6 | BLK | F805 | Ground to G103
7 | BRN/PPL | XY800 | Delayed Interior Lamp Relay Signal
8 | BLK/BLU | FP28 | Fog Lamp Switch Signal
9 | BRN/PPL | XY801 | Interior Lamp Relay Signal
10 | BRN | X820 | B+ from Fuse #15
11 | BRN/BLU | XP810 | Battery Guard Signal
12 | RED | A821 | B+ from Fuse #8
13 | BRN/BLU | XP803 | Rear Compartment Open Signal
14 | RED | A600 | Low Power Drive Signal

#### Park Lamp Relay K130

Connector Part Information |

• | ZFW 5-20

• | 5 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BRN/WHT | XM810 XM815 | Relay Control
2 | -- | -- | Not Used
3 | RED/WHT | AM810 AM811 | Exterior Lamp Power
4 | GRY/GRN | RU812 | Lamp ON Signal
5 | RED | A813 | B+ from Fuse V3

#### RH Backup Lamp

Connector Part Information |

• | PF 2-1

• | 2 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK | F2 | Ground to G400
2 | WHT/BLK | MF1 | Lamp ON Feed

#### RH Cornering Lamp

Connector Part Information |

• | ZFW 2-9

• | 2 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY/RED | RA1 | Lamp ON Signal
2 | BLK | F5 | Ground to G103

#### RH Fog Lamp

Connector Part Information |

• | ZFW 2-10

• | 2 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/BLU | FP3 | Lamp ON Signal
2 | BLK | F4 | Ground to G103

#### RH Front Side Door Jamb Switch

Connector Part Information |

• | F 2-42

• | 2 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | GRY | R6 | Door Open Signal

#### RH Front Side Door Lock Switch

Connector Part Information |

• | F 4-21

• | 4 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/BRN | FX805 | Door Lock Signal
2 | BLK/PPL | FY805 | Door Unlock Signal
3 | RED/BLU | AP807 | Illumination Signal
4 | BLK | F12 | Ground to G200

#### RH Front Side Marker Lamp

Connector Part Information |

• | ZFW 2-9

• | 2 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK/GRN | FU1 | Ground
2 | GRY/GRN | RU3 | Lamp ON Signal

#### RH Headlamp Relay (High Beam) K132

Connector Part Information |

• | ZF 9-14

• | 9 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | RED | A850 | B+ from Fuse #32
3 | -- | -- | Not Used
4 | RED | A827 | B+ from Fuse #32
5 | BLK/RED | FA888 | B+ for Fog Lamps
6 | WHT | M62 | Relay Control
7 | -- | -- | Not Used
8 | WHT | M64 M65 | Lamp On Signal
9 | -- | -- | Not Used

#### RH Headlamp

Connector Part Information |

• | ZPF 5-1

• | 5 Way F

• | BLK

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | BLK | F11 | Ground to G103
C | YEL | B3 | Low Beam Signal
D | -- | -- | Not Used
E | WHT | M1 | High Beam Signal

#### RH Park/Turn Signal Lamp

Connector Part Information |

• | ZFW 3-21

• | 3 Way F

• | GRY

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | F16 | Ground to G103
B | GRY/RED | RA3 | Park Lamp Signal
C | BLK/GRN | FU2 | Park Lamp Signal

#### RH Rear Side Door Jamb Switch

Connector Part Information |

• | F 2-42

• | 2 Way F

• | BLK

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY | R2 | Door Open Signal
2 | GRY | R1 | Door Open Signal

#### RH Rear Side Marker Lamp

Connector Part Information |

• | ZFW 2-9

• | 2 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRY/RED | RA1 | Lamp ON Signal
2 | BLK/GRN | FU1 | Ground

#### RH Stop/Taillamp

Connector Part Information |

• | PF 4-2

• | 4 Way F

• | BLK

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/GRN | FU20 | Lamp ON signal
B | BLK | F25 | Ground to G400
C | GRY/RED | RA4 | Lamp ON Signal
D | BLK/YEL | FB2 | Brake Lamp Signal

#### RH Sunshade Illuminated Mirror Lamp

Connector Part Information |

• | ZPF 2-50

• | 2 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | F1 | Ground to G103
B | RED/BLU | AP1 | B+ from Multifunction Relay

#### Stop Lamp Switch

Connector Part Information |

• | ZF 4-6

• | 4 Way F

• | BLK

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RED | A401 | B+ from Fuse #12
2 | BLK/YEL | FB101 | Brake Lamp ON Signal
3 | BRN | X120 | B+ from Fuse #2
4 | BLK/BRN | FX102 | BTSI Signal

#### Taillamp (Middle)

Connector Part Information |

• | ZPF 2-50

• | 2 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | F4 | Ground to G400
B | GRY/BLK | RF1 | Lamp ON Signal

#### Turn Signal Lamp Flasher K10

Connector Part Information |

• | ZF 9-14

• | 9 Way F

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-3 | -- | -- | Not Used
4 | BLK | F12 | Ground to G103
5 | -- | -- | Not Used
6 | BLU | P3 | Ignition Voltage
7 | -- | -- | Not Used
8 | BLK/WHT | FM22 FM91 | Lamps ON Signal

#### Turn Signal Switch

Connector Part Information |

• | ZF 10-3

• | 10 Way F

• | BLK

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YEL | B905 | B+ from Fuse #31
2 | WHT | M3 | High Beam ON/OFF Signal
3 | YEL | B800 B905 | B+ from Fuse #31
4 | BLK/WHT | FM91 | Hazard Signal
5 | RED | A8 | B+ from Fuse #8
6 | -- | -- | Not Used
7 | GRY/RED | RA999 | RH Cornering Lamp Signal
8 | BLK/GRN | FU1 | RH Turn Indicator
9 | BLK/WHT | FM1 | LH Turn Indicator
10 | GRY/BLK | RH999 | LH Cornering Lamp Signal