BLUSHING EXTERIOR W/DISPERSION LAQUER PAINT. Cadillac Cimarron 1985

For 1990-2009 cars

# BLUSHING EXTERIOR W/DISPERSION LAQUER PAINT

#### MODELS AFFECTED: 1985 CIMARRON

The exterior paint on some 1985 Cimarrons that were finished with Bordeaux Red (code 79-WA- 8529) Dispersion Lacquer may exhibit a blushing condition. Blushing can best be described as a white hazy or milky discoloration and is evidenced by comparing the appearance of the outside rearview mirrors or soft body fascia to adjacent body parts. This condition is due to paint that was contaminated in the paint manufacturing process. Janesville Assembly Plant from April 11 through July 30, 1985, with VIN Numbers FJ509935 through FJ518610.

A finish that shows blushing can be polished to a high luster, but will show signs of blushing within a few days.

To correct the condition, the entire vehicle must be color coated, except the soft fascia.

#### Repair procedure:

1. Detach all readily removable exterior items (moldings, taillamps, grilles, emblems, etc.).

2. Throughly clean the exterior with a detergent and water followed by a Lacquer and enamel cleaner, (DuPont 3939S or equivalent).

3. Wet sand with 600 or finer paper.

4. Reclean exterior with Lacquer and enamel cleaner (DuPont 3939S or equivalent) and tack off.

5. Apply 3 to 5 coats of acrylic Lacquer (DuPont Lucite, code 79-B8509 or equivalent) so that a minimum film build of 1.0 mil. is maintained after compounding.

6. Allow to dry overnight and compound.

7. Replace all removed exterior items.

For warranty purposes, submit a warranty cliam as follows:

Other Sublet Labor Labor Labor Material Description Operation Hours Hours Towing ----------- --------- ----- ----- -------- Color Coat Entire T0132 13.9 *.4 **111.03 Vehicle (Includes R&R of exterior Trim)

* Paint mix time ** Paint material allowance

#### NOTE: Authorization is required prior to repair. (Zone approval or Dealer approval is qualified under the Dealer Warranty Management System).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.