WATER LEAK AT VISTA VENT IMPROVE SEALING OF VISTA VENT. Cadillac Cimarron 1986

For 1990-2009 cars

# WATER LEAK AT VISTA VENT IMPROVE SEALING OF VISTA VENT

#### MODELS AFFECTED: 1982 THROUGH 1986 CIMARRONS WITH VISTA-VENT OPTION (AD3)

Some 1982 through 1986 Cimarrons equipped with a vista-vent may experience a water leak condition between the vista-vent glass and weatherstrip. This condition may be caused by weak hinges. To correct this condition, replace both hinges with new hardened steel hinge (P/N 20696950).

Any sunroof glass in stock with old style hinges should have the new hinges installed before it is placed in service.

For warranty purposes, use Labor Operation B2227 at .3 hours.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.