THM 125C TRANSMISSION USAGE INFORMATION. Cadillac Cimarron 1984

For 1990-2009 cars

# THM 125C TRANSMISSION USAGE INFORMATION

#### MODELS AFFECTED: 1984 CIMARRONS WITH THM 125C AUTOMATIC TRANSAXLE

Production of the 1984 model Cimarron has been extended into the 1985 model year.

Starting at Broadcast #419885 for model "CB" and Broadcast #420967 for model "CA" transaxles,late 1984 model year Cimarrons will be built with 1985 model THM 125C transaxles. There are differences in service parts between 1984 and 1985 model year THM 125C transaxles. When servicing any 1984 Cimarron equipped with a THM 125C transaxle, verify the model year of the transaxle by looking at the nameplate located on top of the transaxle by the manual shaft (refer to Figure 1).

#### NOTE: If the transaxle being serviced is a 1984 model, you must refer to the 1984 parts list, and if it is a 1985 model, you must refer to the 1985 parts list in order to obtain the correct service parts.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.