Loss of Power. Cadillac Concours 1997

For 1990-2009 cars

Checks | Causes
--- | ---
1-2 and 2-3 Shift Solenoid Valves | 2nd gear starts
Engine Performance | Fuel and or exhaust system concern
TCC System | TCC Stuck ON or dragging

TFP Switch

• | Engine operating in torque management mode

• | Incorrect data input causing the PCM to command torque management mode

• | See DTC table

Torque Converter | Debris
Transmission | Low fluid
Turbine Shaft | Bushing damage