New Thread Repair Kit Available for Damaged Engine Block Bolt Holes. Cadillac Concours 1996

For 1990-2009 cars

# New Thread Repair Kit Available for Damaged Engine Block Bolt Holes

Subject: | New Thread Repair Kit Available For Damaged Engine Block Bolt Holes

Models: | 1993 Cadillac Allante

| 1996-1999 Cadillac Deville

| 1993-1999 Cadillac Eldorado, Seville

| 1994-1999 Cadillac Concours

| 1995-1999 Oldsmobile Aurora

| 1999 Marine

| with 4.0 L or 4.6 L Engine (VINs C, Y, 9 -- RPOs L47, LD8, L37)

This bulletin is being revised to remove models. Please discard Corporate Bulletin Number 99-06-01-015 (Section 06 - Engine).

A thread repair kit (Kent-Moore J 42385-500) is available to repair damaged engine block bolt holes for the cylinder head bolts and the crankshaft main bearing bolts. Installation instructions are included with each kit.