Starter and Charging System Check. Cadillac Concours 1997

For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 | Turn the ignition switch to the START position. | Engine cranks. | Starter Solenoid Does Not Click Starter Solenoid Clicks, Engine Does Not Crank
2 | Engine running. | The charging system is operating properly. The volt/charge indicator is operating properly | Battery Is Undercharged or Overcharged Volt/Charge Indicator Always On Volt/Charge Indicator Inoperative
* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.