Automatic Transmission Components. Cadillac Concours 1996

For 1990-2009 cars

#### A/T Controls Component Location Table

Name | Location | Locator View | Connector End View | Group No.
--- | --- | --- | --- | ---
1-2 Shift Solenoid Valve | In transmission valve body | Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
2-3 Shift Solenoid Valve | In transmission valve body | Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
Automatic Transmission Fluid Pressure Manual Valve Position Switch (TFP Val. Position Sw.) | In transmission valve body | Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
Automatic Transmission Fluid Temperature (TFT) Sensor | In transmission valve body | Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
Automatic Transmission Input (Shaft) Speed (A/T ISS) Sensor | In transmission valve body | Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
Brake Switch | Below LH side of IP, above brake pedal | 8A-201-31 Fig. 60 | 8A-202-16 | --
Engine Compartment Fuse/Relay Center | Forward of LH front strut tower | 8A-201-7 Fig. 15 | 8A-11-0 | --
Powertrain control Module (PCM) | LH front corner of engine compartment, under air cleaner housing | 6 - Engine Controls |  | --
C1 (80 cavities) | Engine harness to PCM, LH front corner of engine compartment, under air cleaner housing |  | 6 - Engine Controls | --
C2 (80 cavities) | Engine harness to PCM, LH front corner of engine compartment, under air cleaner housing |  | 6 - Engine Controls | --
Pressure Control Solenoid Valve (PC SOL. Valve) | In transmission valve body | Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
Torque Converter Clutch Pulse Width Modulation Solenoid (TCC PWM Sol.) Valve | In transmission valve body | Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
Trunk Compartment Fuse Block | In trunk, attached to electronics bay | 8A-201-34 Fig. 66 | 8A-202-8 | --
Vehicle Speed Sensor (VSS) | Lower RH rear of engine on transmission | Automatic Transmission Electronic Component Views | 7 - Automatic Transmission | --
C101 (23 cavities) | Body main harness, LH side of engine compartment, on wheelhouse | 8A-201-7 Fig. 15 | 8A-202-0 | --
C106 (14 cavities) | Engine harness to transmission, LH front of transmission | 7 - Automatic Transmission | 7 - Automatic Transmission | --
P101 | LH rear corner of engine, on cowl | 8A-201-29 Fig. 56 | -- | --
S126 | Engine harness, top LH side of engine about 10.5 cm from connector C127 breakout | 8A-201-18 Fig. 35 | -- | --
S318 | Body main harness about 18 cm (Deville/Concours), or about 31 cm (Eldorado/Seville) from sensing and diagnostic module (SDM) | 8A-201-38 Fig. 73 | -- | --