C/C OR BRAKE/TRANSMISSION SHIFT INTERLOCK (BTSI) INOP.. Cadillac Concours 1994

For 1990-2009 cars

# C/C OR BRAKE/TRANSMISSION SHIFT INTERLOCK (BTSI) INOP.

#### SUBJECT: CRUISE CONTROL OR BRAKE/TRANSMISSION SHIFT INTERLOCK (BTSI) INOPERATIVE (REPLACE LOWER STOPLAMP SWITCH)

#### MODELS: 1994 CADILLAC CONCOURS, DEVILLE, ELDORADO AND SEVILLE WITHIN THE FOLLOWING VIN BREAKPOINTS: DEVILLE AND CONCOURS - SOP TO 207557 ELDORADO - SOP TO 605732 SEVILLE - SOP TO 814612

#### CONDITION:

SOME OWNERS MAY EXPERIENCE AN INOPERATIVE CRUISE CONTROL OR BRAKE/TRANSMISSION SHIFT INTERLOCK (BTSI).

#### CAUSE:

THE CAUSE MAY BE DUE TO A MISADJUSTMENT OF THE STOPLAMP SWITCH ASSEMBLY.

#### CORRECTION:

TO REPAIR THIS CONDITION, REPLACE THE LOWER SWITCH IN THE STOPLAMP SWITCH ASSEMBLY WITH P/N 12450005. FOLLOW THE REPLACEMENT AND ADJUSTMENT PROCEDURES IN SECTION 5 OF THE APPLICABLE SERVICE MANUAL.

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: N2440 USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.