SMU - SECTION 0B - REVISED THROTTLE BODY CLEANING PROC.. Cadillac Concours 1996

For 1990-2009 cars

# SMU - SECTION 0B - REVISED THROTTLE BODY CLEANING PROC.

REVISION: 08/08/96

THIS BULLETIN IS BEING REVISED TO UPDATE THE INSPECTION MILEAGE INTERVALS. PLEASE DISCARD CORPORATE BULLETIN NUMBER 63-02-01 (SECTION 0 - GENERAL INFORMATION). ______________________________________________________________________

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 0B - REVISED THROTTLE BODY INSPECTION MILEAGE INTERVALS AND MAINTENANCE INTERVAL IN CADILLAC AND OLDSMOBILE MAINTENANCE SCHEDULE

#### MODELS: 1996 CADILLAC CONCOURS, DEVILLE, ELDORADO, SEVILLE 1996 OLDSMOBILE AURORA WITH 4.0L AND 4.6L ENGINE (VINS C, Y, 9-RPOS L47, LD8, L37)

THIS BULLETIN IS BEING ISSUED TO REVISE THE THROTTLE BODY INSPECTION INTERVALS IN SECTION 0B (MAINTENANCE AND LUBRICATION) OF THE APPLICABLE SERVICE MANUALS. THESE NEW MILEAGE INTERVALS SHOULD BE USED FOR 1996 VEHICLES WITH 4.0 AND 4.6 LITER V8 ENGINES. INSPECTION IS TO BE PERFORMED AT 15,000 MILES (25 000KM) AND EVERY 30,000 MILES (50 000KM) THEREAFTER.

#### PROCEDURE:

INSPECT THROTTLE BODY BORE AND THROTTLE VALVE PLATE FOR DEPOSITS. REFER TO THROTTLE BODY ASSEMBLY (CLEANING PROCEDURE) IN THE ENGINE CONTROLS SECTION OF THE SERVICE MANUAL (OLDSMOBILE) OR THROTTLE BODY CLEANING PROCEDURE IN THE MAINTENANCE AND LUBRICATION SECTION OF THE SERVICE MANUAL (CADILLAC).

#### CADILLAC ONLY:

THE CADILLAC MAINTENANCE SCHEDULE HAS COUPONS FOR OVER 100,000 MILES (160 000KM) BUT THE THROTTLE BODY INSPECTION IS NOT INCLUDED AFTER 100,000 MILES (160 000KM) ON THOSE COUPONS. STARTING AT 105,000 MILES (169 000KM), THROTTLE BODY INSPECTION EVERY 30,000 MILES (50 000KM).

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.