TOWING MANUAL (T65) UPDATE (REVISED TOWING LIMITS). Cadillac Concours 1994

For 1990-2009 cars

# TOWING MANUAL (T65) UPDATE (REVISED TOWING LIMITS)

********************************************************************** TOWING MANUAL (T65) UPDATE **********************************************************************

#### SUBJECT: TOWING MANUAL (T65) UPDATE - (REVISE TOWING LIMITS)

#### MODELS: 1994 CADILLAC CONCOURS, DEVILLE, ELDORADO AND SEVILLE

THE FOLLOWING CHANGE PERTAINS TO THE 1994 GENERAL MOTORS PASSENGER CAR AND LIGHT DUTY TRUCK TOWING MANUAL (T-65). THE TOW LIMITS ON PAGE 39 ARE INCORRECT FOR THE FOLLOWING VEHICLES. CADILLAC ELDORADO, ELDORADO TOURING COUPE, SEVILLE, SEVILLE STS AND CONCOURS. THE CORRECT TOW LIMITS ARE 35 MPH FOR 25 MILES FOR THESE VEHICLES. THE CADILLAC DEVILLE TOW LIMITS ARE CORRECT, 55 MPH FOR 500 MILES.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.