Part D: Recommended Fluids and Lubricants. Cadillac Evoq 2003

For 1990-2009 cars

Fluids and lubricants identified below by name, part number or specification may be obtained from your dealer.

Usage | Fluid/Lubricant
--- | ---
Engine Oil | The engine requires a special engine oil meeting GM Standard GM4718M. Oils meeting this standard may be identified as synthetic, and should also be identified with the American Petroleum Institute Certified for Gasoline Engines starburst symbol. However, not all synthetic API oils with the starburst symbol will meet this GM standard. You should look for and use only an oil that meets GM Standard GM4718M. For the proper viscosity, see Engine Oil .
Engine Coolant | 50/50 mixture of clean, drinkable water and use only DEX-COOL Coolant. See Engine Coolant .
Hydraulic Brake System | Delco Supreme 11 Brake Fluid or equivalent DOT-3 brake fluid.
Windshield Washer Solvent | GM Optikleen Washer Solvent or equivalent.
Hydraulic Clutch System | Hydraulic Clutch Fluid (GM Part No. U.S. 12345347, in Canada 10953517, or equivalent DOT-3 brake fluid).
Power Steering System | GM Power Steering Fluid (GM Part No.U.S. 1052884, in Canada 993294, or equivalent).
Manual Transmission | DEXRON-III Automatic Transmission Fluid.
Automatic Transmission | DEXRON-III Automatic Transmission Fluid.
Key Lock Cylinders | Multi-Purpose Lubricant, Superlube (GM Part No. U.S. 12346241, in Canada 10953474, or equivalent).
Rear Axle (Limited-Slip Differential) | SAE 75W-90 Synthetic Axle Lubricant (GM Part No. U.S. 12378261, in Canada 10953455, or equivalent) meeting GM Specification 9986115. With a complete drain and refill add 4 ounces (118 ml) of Limited-Slip Axle Lubricant Additive (GM Part No. U.S. 1052358, in Canada 992694, or equivalent) where required. See Rear Axle .
Hood Latch Assembly, Secondary Latch, Pivots, Spring Anchor and Release Pawl | Lubriplate Lubricant Aerosol (GM Part No. U.S. 12346293, in Canada 992723, or equivalent) or lubricant meeting requirements of NLGI #2, Category LB or GC-LB.
Hood and Door Hinges | Multi-Purpose Lubricant, Superlube (GM Part No. U.S. 12346241, in Canada 10953474, or equivalent).
Weatherstrip Conditioning | Dielectric Silicone Grease (GM Part No. U.S. 12345579, in Canada 10953014, or equivalent).