Transfer Case Housings Cleaning and Inspection. Cadillac Evoq 2003

For 1990-2009 cars

1. Clean all case/housings in solvent.
2. Remove all sealant material from the sealing surfaces.
3. Inspect for the following:

• | Damaged gasket sealing surfaces (1)

• | Worn, scored, or loose bearing races or worn bearing race bores (2)

• | Damaged bolt threads (3)

• | Damaged oil seal bores (4)

• | A loose, damaged, or restricted vent tube (5)

• | Damaged speed sensor bore (6)

• | Porosity

• | Damage to the exterior of the case/housings