For 1990-2009 cars

# PROM CALIBRATION/REPLACEMENT UPDATED DIAGNOSTICS

#### SUBJECT: INFORMATION ON PROM CALIBRATIONS

#### MODELS AFFECTED: 1980-1993 ELDORADOS, SEVILLES, AND BROUGHAMS 1982-1988 CIMARRONS 1985 -1993 DE VILLES AND FLEETWOODS 1987-1993 ALLANTES

This bulletin is being issued as a supplement to bulletin T-89-102, Group 6E. This supplement begins with the 1988 D - Car.

This bulletin summarize all 1980 through 1993 C, D, E, K, V, and J gasoline engine PROM calibrations to date. When any diagnosis leads to PROM replacement, the service PROM part number listed should be used. Should any additional PROM calibration changes be made, the GMSPO parts distribution system will automatically supersede these service part numbers.

PROM changes may be made for many different reasons. For instance, a calibration change may be made in conjunction with component changes, for a repair relative to a current field condition, or as a running change to provide minor modifications affecting driveability or fuel economy. Therefore, if a PROM I.D. is lower than the latest PROM available, it does not necessarily need replacement. Refer to the bulletin listed for details about the symptom that may require a PROM change.

Parts are currently available from GMSPO.

1988 D EQUIPPED WITH 5.OL CCC V-8 ENGINE

SERVICE ECM P/N 1228330

Service Latest Production Service PROM Service PROM Broadcast Code Broadcast Code Part I.D. Part Number ------------------------------------------------------------ First Gen.:

D Fed. ADAY ALUP 2182 16122177 D Cal. ADAZ APSW 2057 16132056 D Export ADBA ADBA 7533 16077532

Second Gen.: Bulletin T-89-39 "Insufficient A/C Cooling When Driving".

D Fed. ALUP ALUP 2182 16122177 D Cal. APSW APSW 2057 16132056

1988 J EQUIPPED WITH 2.8L PFI V-6 ENGINE

SERVICE ECM P/N 1227730

First Gen.:

J Fed. Auto. AKDN ANWD 8991 16128936 J Fed. Manual AKDM ANWC 8981 16128934 J Cal. Auto. AKDK ANWB 8971 16128933 J Cal. Manual AKDP ANWF 9001 16128937

Second Gen.: Bulletin T- 89 -17 "Engine Stall, Only After Cold Start, or Idle Surge May Set Code 35".

J Fed. Auto. ANWD ANWD 8991 16128936 J Fed. Manual ANWC ANWC 8981 16128934 J Cal. Auto. ANWB ANWB 8971 16128933 J Cal. Manual ANVF ANWF 9001 16128937

Third Gen: Bulletin T-89-17A "Tip In Hesitation On Acceleration, Engine Stall On Cold Start, or Engine Stall On Deceleration".

J Fed. Auto. ARDC ARDC 4761 16134468 J Fed. Manual ARDB ARDB 4751 16134466 J Cal. Auto. ARDA ARDA 4741 16134465 J Cal. Manual ARDD ARDD 4771 16134482

Fourth Gen.: Bulletin T - 90 - 52 "Tip In Hesitation On Acceleration, Engine Stall On Cold Start, or Engine Stall On Deceleration".

J Fed. Auto. ARDC ARDC 4761 16134468 J Fed. Manual ARDB ATZA 8261 16148227 J Cal. Auto. ARDA ARDA 4741 16134465 J Cal. Manual ARDD ATZB 8271 16148228

1988 C, E, AND K EQUIPPED WITH 4.5L DFI V-8 ENGINE

SERVICE ECM P/N 1228322

Production Service Latest Broadcast Code Broadcast Code Service PROM (PROM I.D.) (PROM I.D.) Part Number ---------------------------------------------------- First Gen.:

C Fed. AKYA (701) AMNS (850) 16089317 C Cal. ADBK (702) AMNT (851) 16089322 ADBP (703) ADBP (703) 16077616 C Limousine Com. Chassis E/K Fed. AKYB (861) AMNP (1000) 16089308 E/K Cal. ADBF (862) AMNR (1001) 16089313 K STS Fed. AMYW (1002) AMYW (1002) 16120924 K STS Cal. AMYX (1003) AMYX (1003) 16120931

Second Gen.: Bulletin T-88-106 "Cruise Control Inoperative Code E67 and/or Cruise Control Resume Does Not Return to Set Speed".

C Fed. AMNS (850) AMNS (850) 16089317 C Cal. AMNT (851) AMNT (851) 16089322 E/K Fed. AMNP (1000) AMNP (1000) 16089308 E/K Cal. AMNR (1003) AMNR (1001) 16089313

1988 V EQUIPPED WITH 4.1L PFI V-8 ENGINE

SERVICE ECM P/N 1227750

First Gen.: V ADBC (545) ADBC (545) 16076500

1989 C, E, AND K EQUIPPED WITH 4.5L DFI V-8 ENGINE

SERVICE ECM P/N 1228322

Production Service Latest Broadcast Code Broadcast Code Service PROM (PROM I.D.) (PROM I.D.) Part Number First Gen.: --------------------------------------------------- C Fed. ALCK (344) ALCK (344) 16086013 C Cal. ALCL (346) ALCL (346) 16121722 C Export ALCN (349) ALCN (349) 16121734 C Com. Chassis ALCM (348) ALCM (348) 16121730 E/K Fed. ALCP (1004) ALCP (1004) 16121738 E/K Cal. ALCR (1006) ALCR (1006) 16121742 E/K Export ALCS (1008) ALCS (1008) 16121746 E/K Fed. Opt. AMZA (1005) AMZA (1005) 16121268 Axle (GX3) E/K Cal. Opt. AMZB (1007) AMZB (1007) 16121273 Axle (GX3)

1989 V EQUIPPED WITH 4.5L PFI V-8 ENGINE

SERVICE ECM P/N 1227750

First Gen.: V ANZR (2002) ANZR (2002) 16129601

1989 D EQUIPPED WITH 5.OL CCC V-8 ENGINE

SERVICE ECM P/N 1228330

Service Latest Production Service PROM Service PROM Broadcast Code Broadcast Code Part I.D. Part Number ----------------------------------------------------------- First Gen.:

D Fed. ALUP ALUP 2178 16122177 D Cal. APSW APSW 2057 16132056

1990 C, E, AND K EQUIPPED WITH 4.5L PFI V-8 ENGINE

SERVICE ECM P/N 16132240

Production Service Service Service Begin End Broadcast Code Broadcast PROM PROM B.P. B.P. PROM I.D. Code Part I.D. P/N ----------------------------------------------------------- First Gen.:

C Fed. 200001 217229 ATNR (357) ATTT 360 16147006 C Cal. 200001 217586 ATNL (353) ATTN 359 16146990 60 Special Cal. 200001 217586 ATNM (354) ATTP 361 16146994 60 Special/ 200001 217229 ATNN (355) ATTR 362 16146998 Com. Fed. E Fed. 600001 600811 ATNP (1012) ATTS 1020 16147002 E Cal. 600001 600776 ATNJ (1013) ATTL 1018 16146980 E Fed./Cal. 600001 600811 ATNH (1014) ATTK 1017 16146975 K Fed. 800001 801006 ATNP (1012) ATTS 1020 16147002 K Cal. 800001 800776 ATNJ (1013) ATTL 1018 16146980 K STS Fed./Cal. 800001 801006 ATNH (1014) ATTK 1017 16146975

Second Gen.: Bulletin T-90-2A "Engine Stall When Vehicle Placed in Gear".

C Fed. 200001 217229 ATNR (357) ATTT 360 16147006 C Cal. 200001 217586 ATNL (353) ATTN 359 16146990 60 Special Cal. 200001 217S86 ATNM (354) ATTP 361 16146994 60 Special/ 200001 217229 ATNN (355) ATTR 362 16146998 Com. Fed. E Fed. 600001 600811 ATNP (1012) ATTS 1020 16147002 E Cal. 600001 600776 ATNJ (1013) ATTL 1018 16146980 E Fed./Cal. 600001 600811 ATNH (1014) ATTK 1017 16146975 K Fed. 800001 801006 ATNP (1012) ATTS 1020 16147002 K Cal. 800001 800776 ATNJ (1013) ATTL 1018 16146980 K STS Fed./Cal. 800001 801006 ATNH (1014) ATTK 1017 16146975

1990 V EQUIPPED WITH 4.5L PFI V-8 ENGINE

SERVICE ECM P/N 16132240

Production Service Latest Broadcast Code Broadcast Code Service PROM PROM I.D. PROM I.D. Part Number First Gen.: -------------------------------------------------- V Fed./Cal. APNF (2006) AUNX (2009) 16151465 V Export APJZ (2007) AUNY (2010) 16151467

Second Gen.: Bulletin T-90-73 "Intermittent Cruise Control Operation".

V Fed./Cal. APNF (2006) AUNX (2009) 16151465 V Export APJZ (2007) AUNY (2010) 16151467

1990 D EQUIPPED WITH 5.OL CCC V-8 ENGINE

SERVICE ECM P/N 1228330

Service Latest Production Service PROM Service PROM Broadcast Code Broadcast Code Part I.D. Part Number First Gen.: ------------------------------------------------------------ D Fed. ALUP ALUP 2178 16122177 D Cal. APSW APSW 2057 16132056

1990 D EQUIPPED WITH 5.7L TBI ENGINE

SERVICE ECM P/N 1228746

Service Latest Production Service PROM Service PROM Broadcast Code Broadcast Code Part I.D. Part Number First Gen.: --------------------------------------------------------- D Fed./Cal. ANXM AUJJ 0521 16151357

Second Gen.: Bulletin T-90-77 "Tip-In Hesitation or Sag, Code 43".

D Fed./Cal. ANXM AUJJ 0521 16151357

1991 C, E, AND K EQUIPPED WITH 4.9L PFI V-8 ENGINE

SERVICE ECM P/N 16132240

Service Service Emission PROM Broadcast Service Vehicle Year System I.D. Code P/N ----------------------------------------------------------------------- First Gen.:

DeVille Coupe, DeVille 1991 Fed. 365 ATCX 16155327 Sedan, Fleetwood Coupe DeVille Coupe, DeVille 1991 Cal. 366 ATCY 16155332 Sedan, Fleetwood Coupe Fleetwood Sedan, 60 Special, 1991 Fed. 368 ATDA 16155425 Funeral Coach Fleetwood Sedan, 60 Special, 1991 Cal. 370 ATRM 16155437 Funeral Coach C Touring Sedan 1991 Fed./Cal. 372 AXTA 16164194 E/K 1991 Fed. 1024 ATCT 16155247 E/K 1991 Cal. 1025 ATCU 16155316 ETC/STS 1991 Fed./Cal. 1028 ATFT 16155429

Second Gen.: Bulletin T-91-81A "Engine Stalling on Coast Down and/or ECM Codes E22, E26, E32, E55, E70, or E85".

DeVille Coupe, DeVille 1991 Fed. 384 AYFP 16164699 Sedan, Fleetwood Coupe DeVille Coupe, DeVille 1991 Cal. 385 AYFR 16164700 Sedan, Fleetwood Coupe Fleetwood Sedan, 60 Special, 1991 Fed. 387 AYFT 16164702 Funeral Coach Fleetwood Sedan, 60 Special 1991 Cal. 388 C Touring Sedan 1991 Fed./Cal. 383 AYFH 16164692 E/K 1991 Fed. 1041 AYKM 16165502 E/K 1991 Cal. 1042 AYKN 16165507 ETC/STS 1991 Fed./Cal. 1043 AYKP 16165511

1991 C, E, AND K EQUIPPED WITH 4.9L PFI V-8 ENGINE

SERVICE ECM P/N 16132240

Service Service Emission PROM Broadcast Service Vehicle Year System I.D. Code P/N ------------------------------------------------------------------------- Third Gen.: Bulletin T-91-81B "Engine Stalling on Coast Down, Cold Hesitation, and/or ECM Codes E22, E26, E32, E55, E70, or E85".

DeVille Coupe, DeVille 1991 Fed. 395 AZPW 16171872 Sedan, Fleetwood Coupe DeVille Coupe, DeVille 1991 Cal. 398 AZCT 16169080 Sedan, Fleetwood Coupe Fleetwood Sedan, 60 Special, 1991 Fed. 397 AZCU 16169095 Funeral Coach Fleetwood Sedan, 60 Special 1991 Cal. 396 AZPX 16171877 C Touring Sedan 1991 Fed./Cal. 402 AZCX 16169105 E/K 1991 Fed. 1054 AZWZ 16172096 E/K 1991 Cal. 1055 AZXA 16172103 ETC/STS 1991 Fed./Cal. 1056 AZXB 16172110

Fourth Gen.: Bulletin T-93-44 "Intermittent Stall After Start Cold, Engine Stalling on Coast Down, Hesitation Cold, or ECM Codes E22, E26, E32, E55, E70, and/or E85".

DeVille Coupe, DeVille 1991 Fed. 417 BBXF 16180314 Sedan, Fleetwood Coupe DeVille Coupe, DeVille 1991 Cal. 418 BBXH 16180315 Sedan, Fleetwood Coupe Fleetwood Sedan, 60 Special, 1991 Fed. 421 BBXL 16180320 Funeral Coach Fleetwood Sedan, 60 Special 1991 Cal. 419 BBXJ 16180317 C Heavy-Duty Chassis 1991 Fed./Cal. 420 BBXK 16180318 C Touring Sedan 1991 Fed./Cal. 416 BBXC 16180312 E/K 1991 Fed. 1065 BBWW 16180302 E/K 1991 Cal. 1066 BBWX 16180303 ETC/STS 1991 Fed./Cal. 1067 BBWY 16180304

1991 V EQUIPPED WITH 4.5L PFI V-8 ENGINE

SERVICE ECM P/N 16132240

Production Service Latest Broadcast Code Broadcast Code Service PROM (PROM I.D.) (PROM I.D.) Part Number First Gen.: ---------------------------------------------------

V Nat. AUMF (2012) AUMF (2012) 16155445 V Export AUMD (2011) AUMD (2011) 16155441

1991 D EQUIPPED WITH 5.OL TBI V-8 ENGINE

SERVICE ECM P/N 16136965

Service Latest Production Service PROM Service PROM Broadcast Code Broadcast Code Part I.D. Part Number ------------------------------------------------------------ First Gen.:

D Fed./Cal. AWDD AWDD 4828 16154827

Second Gen.: Bulletin T-92-61A "Tip-In Hesitation, Sag, Long Crank Times When Cold, and/or Detonation".

D Fed./Cal. AWDD AXHR 0531 16160477

1991 D EQUIPPED WITH 5.7L TBI V-8 ENGINE

SERVICE ECM P/N 16136965

Service Latest Production Service PROM Service PROM Broadcast Code Broadcast Code Part I.D. Part Number ---------------------------------------------------------- First Gen.:

D Fed./Cal. AWDF AWDF 4833 16154832 D Export (leaded) ASLK ASLK 1899 16141898

Second Gen.: Bulletin T-92-61A "Tip-In Hesitation, Sag, Long Crank Times When Cold, and/or Detonation".

D Fed./Cal. AWDF AXDA 9971 16159963 D Export (leaded) ASLK AXDF 9984 16159983

1992 C, E, AND K EQUIPPED WITH 4.9L PFI V-8 ENGINE

SERVICE ECM P/N 16132240

Service Service Emission PROM Broadcast Service Vehicle Year System I.D. Code P/N ---------------------------------------------------------------------- First Gen.:

DeVille Coupe, DeVille 1992 Fed. 393 AZCS 16171872 Sedan, Fleetwood Coupe DeVille Coupe, DeVille 1992 Cal. 385 AYFR 16169080 Sedan, Fleetwood Coupe Fleetwood Sedan, 60 Special, 1992 Fed. 387 AYFT 16189085 Funeral Coach Fleetwood Sedan, 60 Special 1992 Cal. 392 AZCW 16171877 C Heavy-Duty Chassis 1992 Fed./Cal. 389 AYFW 16169095 C Touring Sedan 1992 Fed./Cal. 383 AYFH 16169105 E/K 1992 Fed. 1044 AYFJ 16169055 E/K 1992 Cal. 1045 AYFK 16169062 ETC/STS 1992 Fed./Cal. 1047 AYFM 16169068

Second Gen.: Bulletin T-93-44 "Intermittent Stall After Start Cold, Engine Stalling On Coast Down, Hesitation Cold, or ECM Codes E22, E26, E32, E55, E70, and/or E85".

DeVille Coupe, DeVille 1992 Fed. 417 BBXF 16180314 Sedan, Fleetwood Coupe DeVille Coupe, DeVille 1992 Cal. 418 BBXH 16180315 Sedan, Fleetwood Coupe Fleetwood Sedan, 60 Special, 1992 Fed. 421 BBXL 16180320 Funeral Coach Fleetwood Sedan, 60 Special 1992 Cal. 419 BBXJ 16180317 C Heavy-Duty Chassis 1992 Fed./Cal. 420 BBXK 16180318 C Touring Sedan 1992 Fed. 416 BBXC 16180312 C Touring Sedan 1992 Cal. 415 BBXB 16180310 E/K 1992 Fed. 1068 BBWZ 16180307 E/K 1992 Cal. 1069 BBXA 16180308 ETC/STS 1992 Fed./Cal. 1070 BBXD 16180313

1992 V EQUIPPED WITH 4.5L PFI V-8 ENGINE

SERVICE ECM P/N 16132240

Production Service Latest Broadcast Code Broadcast Code Service PROM (PROM I.D.) (PROM I.D.) Part Number ----------------------------------------------------- First Gen.:

V Nat. AUMF (2012) AUMF (2012) 16155445 V Export AUMD (2011) AUMD (2011) 16155441

1992 D EQUIPPED WITH 5.OL TBI V-8 ENGINE

SERVICE ECM P/N 16136965

Service Latest Production Service PROM Service PROM Broadcast Code Broadcast Code Part I.D. Part Number ----------------------------------------------------------- First Gen,:

D Fed./Cal. AXHR AXHR 0531 16160477

1992 D EQUIPPED WITH 5.7L TBI V-8 ENGINE

SERVICE ECM P/N 16136965

Service Latest Production Service PROM Service PROM Broadcast Code Broadcast Code Part I.D. Part Number -------------------------------------------------------- First Gen.:

D Fed./Cal. AXDA AXDA 9971 16195060 D Export (leaded) AXDF AXDF 9984 16195064

1993 C, E, AND K EQUIPPED WITH 4.9L PFI V-8 ENGINE

SERVICE ECM P/N 16132240

Service Service Emission PROM Broadcast Service Vehicle Year System I.D. Code P/N ----------------------------------------------------------------------- First Gen.: DeVille Coupe, DeVille 1993 Fed. 422 AZXF 16182052 Sedan, Fleetwood Coupe DeVille Coupe, DeVille 1993 Cal. 423 AZXH 16182058 Sedan, Fleetwood Coupe Fleetwood Sedan, 60 Special, 1993 Fed. 424 AZXJ 16182063 Funeral Coach Fleetwood Sedan, 60 Special 1993 Cal. 425 AZXK 16182067 C Heavy Duty 1993 Fed./Cal. 426 AZXL 16182047 C Touring Sedan 1993 Fed. 427 AZXM 16182071 C Touring Sedan 1993 Cal. 428 AZXN 16182075 E/K 1993 Fed. 1071 AZXS 16182079 E/K 1993 Cal. 1072 AZXT 16182083 E/K Leaded 1993 Export 1057 AZXU 16177389

1993 E, K, AND V EQUIPPED WITH 4.6L PFI V-8 ENGINE

SERVICE ECM P/N 16159277 (V W/0 V4J OPTION) SERVICE ECM P/N 16180517 (E/K/V WITH 4.6L)

Service Service Emission PROM Broadcast Service Vehicle Year System I.D. Code P/N ---------------------------------------------------------------------- First Gen.:

E Sport Coupe 1993 Fed. 1106/ BBSW 16180899 1306 E Touring Coupe w/o 1993 Fed./Cal. 1103/ BCCK 16181603 Heated Windshield 1304 E Touring Coupe with 1993 Fed./Cal. 1103/ BCCJ 16181599 Heated Windshield 1303 K STS w/o Heated 1993 Fed./Cal. 1104/ BCCL 16181615 Windshield 1304 K STS with Heated 1993 Fed./Cal. 1104/ BCCM 16181623 Windshield 1303 E/K Leaded 1993 Export 1104/ BBSX 16180915 1305 V w/o V4J Option 1993 Fed./Cal. 2103/ AZYC 16179000 2304

Second Gen.:

V with V4J Option 1993 Fed./Cal. 2103/ AZYD 16179000 2305

1993 D EQUIPPED WITH 5.7L TBI V-8 ENGINE

SERVICE ECM P/N 16159280

Service Emission Scanner Broadcast Service Vehicle Year System I.D. Code P/N ----------------------------------------------------------------------- First Gen: Fleetwood, Fleetwood 1993 Fed. 3436 AUKD 16163435 Brougham Fleetwood, Fleetwood 1993 Cal. 0679 AWJN 16170678 Brougham Fleetwood, Fleetwood 1993 Fed./Cal. 4646 AXMN 16164644 Brougham w/Armor Pkg. Fleetwood, Fleetwood 1993 Fed. 4636 AXML 16164634 Brougham w/hearse Conv. Fleetwood, Fleetwood 1993 Cal. 4640 AXMM 16164639 Brougham w/hearse Conv. Fleetwood, Fleetwood 1993 Fed. 0675 AWJM 16170674 Brougham w/Trailer Tow Pkg. Fleetwood, Fleetwood 1993 Cal. 0684 AWJP 16170683 Brougham w/Trailer Tow Pkg.

Second Gen.: Fleetwood, Fleetwood 1993 Fed. 3741 BFYU 16193871 Brougham Fleetwood, Fleetwood 1993 Cal. 3771 BFYY 16193886 Brougham Fleetwood, Fleetwood 1993 Fed./Cal. 3751 BFYN 16193876 Brougham w/Armor Pkg. Fleetwood, Fleetwood 1993 Fed. 3791 BFZA 16193889 Brougham w/Hearse Conv. Fleetwood, Fleetwood 1993 Cal. 3801 BFZB 16193923 Brougham w/Hearse Conv. Fleetwood, Fleetwood 1993 Fed. 3761 BFYX 16193882 Brougham w/Trailer Tow Pkg. Fleetwood, Fleetwood 1993 Cal. 3781 BFYZ 16193919 Brougham w/Trailer Tow Pkg.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.