For 1990-2009 cars

# INTERMITTENT OPER. OF REMOTE KEYLESS ENTRY (RKE)

#### SUBJECT: INTERMITTENT OPERATION OF REMOTE KEYLESS ENTRY (RKE) IN VERY COLD TEMPERATURES (REPLACE MODULE ASSEMBLY)

#### MODELS: 1993 CADILLAC FLEETWOOD BROUGHAM 1994 CADILLAC FLEETWOOD

#### CONDITION:

THE RKE MAY BE INTERMITTENT AT TEMPERATURES BELOW 20 DEGREES F (-29 DEGREES C). OPERATION SHOULD RETURN TO NORMAL AT HIGHER TEMPERATURES.

#### CAUSE:

AN INTERNAL CONDITION IN THE MODULE DOES NOT ALLOW THE MODULE TO RECEIVE THE SIGNAL FROM THE TRANSMITTER.

#### CORRECTION:

REPLACE THE MODULE WITH NEW P/N 10269728, FOLLOWING THE INSTRUCTIONS IN THE SERVICE MANUAL, SECTION 9K. REMEMBER THAT AFTER THE MODULE IS REPLACED, **BOTH** TRANSMITTERS MUST BE REPROGRAMMED AT THE SAME TIME.

#### PART AVAILABILITY:

PARTS ARE EXPECTED TO BE AVAILABLE ON 10/10/94 AT GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE: LABOR OPERATION: R4480 USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.