For 1990-2009 cars

# INFO. REFERENCE CHART FOR A/C COMPRESSOR SEAL WASHERS

#### SUBJECT: INFORMATION - REFERENCE CHART FOR A/C COMPRESSOR SEAL WASHERS

#### MODELS: 1997 AND PRIOR PASSENGER CARS (EXCEPT CORVETTE AND GEO) 1997 AND PRIOR LIGHT DUTY TRUCKS (EXCEPT TRACKER)

GMSPO A/C COMPRESSORS INCLUDE A SEAL WASHER KIT. THESE KITS CONTAIN VARIOUS COLOR EDGE PAINTED WASHER SEALS AND INSERTS IN WHICH ONLY TWO (2) WASHERS AND POSSIBLY ONE (1) INSERT ARE USED. IT HAS COME TO OUR ATTENTION THAT SOME PACKAGING DISCREPANCIES WERE FOUND AND SOME OF THE SEALS CANNOT BE PROPERLY IDENTIFIED FOR INSTALLATION.

THESE SEALS ARE VERY CLOSE IN SIZE AND SOME OF THE SEALS WERE INADVERTENTLY EDGE PAINTED THE WRONG COLOR OR NOT PAINTED.

THE ATTACHED CHART WILL HELP TO PROPERLY IDENTIFY THE SEALS. USE THE ATTACHED CHART BY PLACING THE SEAL OVER THE PICTURED SEAL TO IDENTIFY INSIDE AND OUTSIDE DIAMETERS AND THICKNESS. BECAUSE THESE SEALS ARE VERY SIMILAR IN SIZE, SPECIFICATIONS ARE ALSO LISTED IN THE CHART.

#### IMPORTANT:

IF SEALS ARE DAMAGED UPON INSTALLATION, OBTAIN NEW SEAL KIT. SEALS WILL BE AVAILABLE SEPARATELY AT A LATER DATE.

FIGURES: 00 ATTACHMENTS: 02

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.