For 1990-2009 cars

# NOISE FROM THE FUEL TANK (REPLACE FUEL TANK)

#### MODELS AFFECTED: 1988-1989 BROUGHAMS

Some 1988-1989 Broughams may exhibit a noise from the fuel tank which may be noted when the rear wheels contact a speed bump, railroad tracks, or a pothole. This condition may be caused by "oil canning" of the fuel tank.

To address this condition, strengthening ribs have been added to the fuel tank lower half. To repair this condition install fuel tank, P/N 10174964.

Part is currently available from GMSPO.

WARRANTY INFORMATION VEHICLE SERIES Operation Operation Description Number C D E J K V --------------------- ------ - - -- - - - Tank, Fuel - Replace L1260 .7

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.